Project Name:	CAN
	Project Code:	CAN	Site ID:	C119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	H.M. Churchwood	Locality:	Townsend County Parish Morago portion 60 - mid 
	flood plain of prior stream
	Date Desc.:	25/04/55	Elevation:	 120 metres
	Map Ref.:	Sheet No. : 7827   1:100000	Rainfall:	410
	Northing/Long.:	144.766666666667	Runoff:	Slow
	Easting/Lat.:	-35.4166666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Flood plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Level
	Slope:	<1 % 	Aspect:	125 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Subnatric Grey Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Grey-brown 
	All necessary analytical data are available.	calcareous soil
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Sod grass, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - Eucalytpus largiflorens
	Surface Coarse Fragments:
	Profile Morphology
	A1A2	0 - 0.06 m	Greyish brown (2.5Y5/2-Moist); , 10YR63, 20-50% , 15-30mm; Sandy loam; Weak grade of 
	structure, 10-20 mm, Platy; Dry; Firm consistence; Field pH 6.5 (pH meter); 
	B2	0.06 - 0.15 m	Dark greyish brown (10YR4/2-Moist); ; Heavy clay; 20-50 mm, Angular blocky; Moderate grade of 
	structure, 50-100 mm, Prismatic; Dry; Strong consistence; Field pH 8.2 (pH meter); Clear, Wavy 
	change to - 
	B2	0.15 - 0.3 m	Dark greyish brown (10YR4/2-Moist); ; Heavy clay; 20-50 mm, Angular blocky; Moderate grade of 
	structure, 100-200 mm, Prismatic; Dry; Strong consistence; Common (10 - 20 %), Ferruginous, , 
	Nodules; Very few (0 - 2 %), Calcareous, Very coarse (20 - 60 mm), Concretions; Field pH 8.9 
	(pH meter); 
	0.3 - 0.55 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Strong consistence; Few cutans, <10% of ped faces or walls coated, distinct; 
	Few (2 - 10 %), Calcareous, Very coarse (20 - 60 mm), Concretions; Field pH 8.8 (pH meter); 
	0.55 - 0.7 m	Light brownish grey (2.5Y6/3-Moist); , 2.5Y63, 2-10% ; , 5YR56, 2-10% ; Medium heavy clay; 
	Weak grade of structure, 20-50 mm, Angular blocky; Firm consistence; Few (2 - 10 %), 
	Calcareous, Very coarse (20 - 60 mm), Concretions; Very few (0 - 2 %), Gypseous, Fine (0 - 2 
	mm), Soft segregations; Field pH 8.2 (pH meter); 
	0.7 - 0.84 m	Light brownish grey (2.5Y6/2-Moist); , 2.5Y64, 20-50% ; , 20-50% ; Medium heavy clay; Moderate 
	grade of structure, 20-50 mm, Angular blocky; Very firm consistence; Common cutans, 10-50% 
	of ped faces or walls coated, distinct; Few (2 - 10 %), Calcareous, Very coarse (20 - 60 mm), 
	Concretions; Few (2 - 10 %), Gypseous, Medium (2 -6 mm), Soft segregations; Field pH 8.4 (pH 
	meter); Gradual change to - 
	0.84 - 1.07 m	Light brownish grey (2.5Y6/2-Moist); , 2.5Y63, 20-50% ; , 20-50% ; Medium heavy clay; Strong 
	grade of structure, 50-100 mm, Angular blocky; Firm consistence; Very few (0 - 2 %), 
	Calcareous, Very coarse (20 - 60 mm), Concretions; Few (2 - 10 %), Gypseous, Fine (0 - 2 mm), 
	Soft segregations; Field pH 8.5 (pH meter); 
	Morphological Notes
	Observation Notes

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Notes
	DENIMEIN
	PLEISTOCENE RIVERINE DEPOSIT                                                                                            

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	6.5A	 0.054A	 3.8K	 3.3	 1.4	 0.11	 4.38E	 8.6B
	0.06 - 0.15	8.2A	 0.077A	 9.1K	 10.6	 1.7	 2.3	 2.17E	 23.7B
	0.15 - 0.3	8.9A	 0.1A
	0.3 - 0.55	8.8A	 1.23A
	0.55 - 0.7	8.2A	 1.92A
	0.7 - 0.84	8.4A	 1.95A
	0.84 - 1.07	8.5A	 1.77A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 1.04D	 0.046D	 0.109B	 34D	 32	 22	 12
	0.06 - 0.15	 0.58D	 0.048D	 0.058B	 19D	 20	 12	 49
	0.15 - 0.3	 15D	 22	 14	 49
	0.3 - 0.55	 21D	 23	 14	 40
	0.55 - 0.7	 25D	 20	 19	 36
	0.7 - 0.84	 25D	 21	 22	 32
	0.84 - 1.07	 27D	 22	 15	 36
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.15
	0.15 - 0.3
	0.3 - 0.55
	0.55 - 0.7
	0.7 - 0.84
	0.84 - 1.07

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance