Project Name:	CAN
	Project Code:	CAN	Site ID:	C137	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	H.M. Churchwood	Locality:	Parish Speewa 310M north of south boundary 440M 
	east of west boundary:portion21
	Date Desc.:	01/11/56	Elevation:	 85 metres
	Map Ref.:	Sheet No. : 7627   1:100000	Rainfall:	325
	Northing/Long.:	143.6	Runoff:	Slow
	Easting/Lat.:	-35.2166666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Rolling plains <9m 10-32%	Pattern Type:	Plain
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endohypersodic Regolithic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Tall Strata - Malle shrub, , . *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A2k	0 - 0.1 m	Light brownish grey (10YR6/2-Moist); , 7.5YR54; Light clay; 10-20 mm, Angular blocky; Weak 
	grade of structure, 20-50 mm, Angular blocky; Dry; Weak consistence; Field pH 8.3 (pH meter); 
	A	0.1 - 0.18 m	Light brownish grey (10YR6/2-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Dry; Weak consistence; Field pH 8.6 (pH meter); 
	AB	0.18 - 0.24 m	Greyish brown (10YR5/2-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Moderately moist; Weak consistence; Very few (0 - 2 %), Calcareous, , Concretions; 
	Field pH 8.8 (pH meter); 
	Bk	0.24 - 0.32 m	Pale brown (10YR6/3-Moist); ; Light medium clay; 10-20 mm, Angular blocky; Moderate grade of 
	structure, 20-50 mm, Angular blocky; Moderately moist; Weak consistence; Common (10 - 20 
	%), Calcareous, , Soft segregations; Field pH 9.1 (pH meter); 
	Bk	0.32 - 0.39 m	Pinkish grey (7.5YR6/2-Moist); ; Medium clay; 10-20 mm, Angular blocky; Weak grade of 
	structure, 20-50 mm, Angular blocky; Moderately moist; Weak consistence; Common (10 - 20 
	%), Calcareous, , Concretions; Field pH 9.3 (pH meter); 
	Bk	0.43 - 0.51 m	Brown (7.5YR5/4-Moist); , 10YR52, 10-20% ; , 10-20% ; Medium clay; 10-20 mm, Angular blocky;
	 Weak grade of structure, 20-50 mm, Angular blocky; Dry; Weak consistence; Few cutans, <10%
	 of ped faces or walls coated; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 
	9.5 (pH meter); 
	0.51 - 0.6 m	Brown (7.5YR5/4-Moist); , 10YR52, 2-10% ; , 2-10% ; Medium clay; Weak grade of structure, 20-
	50 mm, Angular blocky; Weak consistence; Few cutans, <10% of ped faces or walls coated; 
	Common (10 - 20 %), Calcareous, , Concretions; Field pH 9.6 (pH meter); 
	0.6 - 0.67 m	Brown (7.5YR5/4-Moist); , 5YR68, 2-10% ; , 2-10% ; Medium clay (Heavy); Weak grade of 
	structure, 20-50 mm, Angular blocky; Weak consistence; Few cutans, <10% of ped faces or 
	walls coated; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 9.5 (pH meter); 
	0.76 - 0.86 m	Light red (2.5YR6/8-Moist); , 5YR54, 20-50% ; , 20-50% ; Medium clay (Heavy); Moderate grade of
	 structure, 10-20 mm, Subangular blocky; Weak consistence; Few cutans, <10% of ped faces or
	 walls coated; Common (10 - 20 %), Calcareous, , Concretions; Field pH 9.3 (pH meter); 

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C137	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	0.86 - 1.09 m	Red (2.5YR5/8-Moist); , 10YR48, 2-10% ; , 2-10% ; Medium clay (Heavy); Moderate grade of 
	structure, 10-20 mm, Subangular blocky; Weak consistence; Common cutans, 10-50% of ped 
	faces or walls coated; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 9 (pH 
	meter); 
	1.19 - 1.3 m	Red (2.5YR5/8-Moist); , 2.5YR46, 2-10% ; , 10YR44, 2-10% ; Medium heavy clay (Heavy); , 
	Subangular blocky; Moderate grade of structure, 10-20 mm, Subangular blocky; Weak 
	consistence; Common cutans, 10-50% of ped faces or walls coated; Common (10 - 20 %), 
	Gypseous, , Concretions; Field pH 9 (pH meter); 
	1.57 - 1.85 m	Red (2.5YR4/6-Moist); ; Medium heavy clay (Heavy); Weak consistence; Common cutans, 10-
	50% of ped faces or walls coated; Common (10 - 20 %), Gypseous, , Soft segregations; Field 
	pH 8.9 (pH meter); 
	1.85 - 2.41 m	Light grey (5Y7/2-Moist); , 7.5YR68, 10-20% ; , 10R58, 10-20% ; Heavy clay; Firm consistence; 
	Common cutans, 10-50% of ped faces or walls coated; Common (10 - 20 %), Gypseous, , 
	Concretions; Field pH 8.8 (pH meter); 
	3.05 - 3.2 m	Reddish yellow (7.5YR6/8-Moist); , 10R48, 2-10% ; , 7.5YR68, 2-10% ; Sandy medium clay 
	(Heavy); Weak consistence; Common cutans, 10-50% of ped faces or walls coated; Field pH 
	7.6 (pH meter); 
	3.58 - 3.81 m	Reddish yellow (7.5YR6/8-Moist); , 10R48, 2-10% ; , 7.5YR68, 2-10% ; Sandy medium clay 
	(Heavy); Firm consistence; Common cutans, 10-50% of ped faces or walls coated; Field pH 7.9 
	(pH meter); 
	4.55 - 4.72 m	Pinkish grey (7.5YR7/2-Moist); , 10YR48, 10-20% ; , 10YR66, 10-20% ; Sandy medium clay 
	(Heavy); Firm consistence; Common cutans, 10-50% of ped faces or walls coated; Field pH 5.8 
	(pH meter); 
	5.03 - 5.18 m	Pinkish grey (7.5YR7/2-Moist); , 10YR48, 10-20% ; , 10YR66, 10-20% ; Sandy medium clay 
	(Heavy); Very firm consistence; Field pH 7 (pH meter); 
	5.38 - 5.54 m	Pinkish grey (7.5YR7/2-Moist); , 10YR48; , 10YR66; Medium heavy clay; Field pH 5.6 (pH meter);
	 
	Morphological Notes
	K4
	Observation Notes
	K2 PARNA:VESICULAR TO 50CM                                                                                              
	Site Notes
	MURRAKOOL

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C137	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.3A	 0.119A	 21K	 4.2	 3.7	 0	 1.5E	 30.4B
	0.1 - 0.18	8.6A	 0.119A	 24.8K	 5.8	 3.2	 0.12	 33.9B
	0.18 - 0.24	8.8A	 0.149A	 25K	 5.7	 1.9	 0.76	 33.4B
	0.24 - 0.32	9.1A	 0.208A	 19.6K	 9.2	 1.3	 1.9	 32B
	0.32 - 0.39	9.3A	 0.238A	 15.5K	 10.5	 1.1	 2.7	 29.8B
	0.43 - 0.51	9.5A	 0.298A
	0.51 - 0.6	9.6A	 0.357A
	0.6 - 0.67	9.5A	 5.36A
	0.76 - 0.86	9.3A	 0.804A
	0.86 - 1.09	9A	 1.4A
	1.19 - 1.3	9A	 1.67A
	1.57 - 1.85	8.9A	 2.17A
	1.85 - 2.41	8.8A	 2.44A
	3.05 - 3.2	7.6A	 2.14A
	3.58 - 3.81	7.9A	 2.23A
	4.55 - 4.72	5.8A	 2.02A
	5.03 - 5.18	7A	 2.38A
	5.38 - 5.54	5.6A	 2.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.15A	 23D	 29	 23	 25
	0.1 - 0.18	 0.22A	 17D	 28	 26	 29
	0.18 - 0.24	 0.54A	 18D	 22	 23	 37
	0.24 - 0.32	 7.04A	 16D	 23	 15	 46
	0.32 - 0.39	 10.6A	 17D	 21	 18	 44
	0.43 - 0.51
	0.51 - 0.6	 17.6A	 16D	 18	 13	 53
	0.6 - 0.67	 19.7A	 16D	 17	 14	 53
	0.76 - 0.86	 31.1A	 18D	 20	 34	 28
	0.86 - 1.09	 23D	 23	 13	 41
	1.19 - 1.3	 23A	 28D	 24	 12	 36
	1.57 - 1.85	 12.8A	 28D	 23	 13	 36
	1.85 - 2.41	 18D	 21	 14	 47
	3.05 - 3.2	 8D	 31	 18	 43
	3.58 - 3.81	 5D	 35	 20	 40
	4.55 - 4.72
	5.03 - 5.18	 5D	 40	 21	 34
	5.38 - 5.54	 4D	 30	 23	 43
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.18
	0.18 - 0.24
	0.24 - 0.32
	0.32 - 0.39

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C137	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	0.43 - 0.51
	0.51 - 0.6
	0.6 - 0.67
	0.76 - 0.86
	0.86 - 1.09
	1.19 - 1.3
	1.57 - 1.85
	1.85 - 2.41
	3.05 - 3.2
	3.58 - 3.81
	4.55 - 4.72
	5.03 - 5.18
	5.38 - 5.54

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C137	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance