Project Name:	CAN
	Project Code:	CAN	Site ID:	C141	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	H.M. Churchwood	Locality:	Parish Speewa portion 22 on south boundary 350M 
	from east boundary
	Date Desc.:	01/12/56	Elevation:	 85 metres
	Map Ref.:	Sheet No. : 7627   1:100000	Rainfall:	325
	Northing/Long.:	143.583333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-35.2	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Petroclcic Hypernatric Red Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Tall Strata - Malle shrub, , . *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Reddish yellow (7.5YR6/6-Moist); ; Sand; Massive grade of structure; Dry; Firm consistence; 
	Field pH 7.6 (pH meter); 
	A2	0.2 - 0.3 m	Reddish yellow (7.5YR6/6-Moist); ; Sand; Massive grade of structure; Dry; Firm consistence; 
	Field pH 8.9 (pH meter); 
	B1	0.36 - 0.46 m	Yellowish red (5YR4/5-Moist); ; Sandy light clay; Weak grade of structure, 50-100 mm, 
	Prismatic; Moderately moist; Weak consistence; Field pH 8.9 (pH meter); 
	B2	0.61 - 0.74 m	Yellowish red (5YR4/6-Moist); , 5YR48, 20-50% ; , 20-50% ; Sandy light clay (Heavy); Moderately 
	moist; Weak consistence; Field pH 9.2 (pH meter); 
	Bk	0.97 - 1.07 m	Yellowish red (5YR5/7-Moist); , 5YR68, 20-50% ; , 20-50% ; Sandy light clay (Heavy); Moderately 
	moist; Weak consistence; Calcrete, Strongly cemented, Discontinuous; Field pH 9.2 (pH 
	meter); 
	Bk	1.27 - 1.37 m	Yellowish red (5YR5/8-Moist); , 5YR68, 20-50% ; , 20-50% ; Sandy light clay (Heavy); Moderately 
	moist; Weak consistence; Calcrete, Very strongly cemented, Discontinuous; Field pH 9.2 (pH 
	meter); 
	D	1.42 - 1.52 m	Yellowish red (5YR5/8-Moist); , 5YR48, 20-50% ; , 20-50% ; Light medium clay; Moderately 
	moist; Weak consistence; Calcrete, Very strongly cemented, Discontinuous; 
	1.6 - 1.68 m	Yellowish red (5YR5/8-Moist); , 5YR48, 20-50% ; , 20-50% ; Light clay (Heavy); Weak 
	consistence; Calcrete, Strongly cemented, Discontinuous; Field pH 9.3 (pH meter); 
	2.06 - 2.13 m	Yellowish red (5YR5/8-Moist); , 5YR48; Light clay (Heavy); Weak consistence; Calcrete, 
	Strongly cemented, Discontinuous; Field pH 9.3 (pH meter); 
	2.69 - 2.79 m	Yellowish red (5YR5/8-Moist); , 5YR48; Light clay (Heavy); Weak consistence; Calcrete, 
	Moderately cemented, Discontinuous; 
	Morphological Notes
	Observation Notes
	K1 ON K2:VESICULAR THROUGHOUT 13MM BLEACHED ZONE AT BOTTOM OF A TOP OF B1                                               

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C141	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Notes
	MURRAKOOL

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C141	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	7.6A	 0.06A
	0.2 - 0.3	8.9A	 0.06A	 2.3K	 1.5	 0.34	 0.85	 5B
	0.36 - 0.46	8.9A	 0.3A	 3.3K	 4.6	 0.45	 3.8	 12.2B
	0.61 - 0.74	9.2A	 0.952A
	0.97 - 1.07	9.2A	 1.52A	 3.6K	 6.2	 0.85	 4.1	 14.8B
	1.27 - 1.37	9.2A	 1.55A
	1.42 - 1.52
	1.6 - 1.68	9.3A	 1.34A
	2.06 - 2.13	9.3A	 1.37A
	2.69 - 2.79
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 51D	 37	 6	 7
	0.2 - 0.3	 0.02A	 55D	 34	 4	 7
	0.36 - 0.46	 0.09A	 40D	 27	 3	 23
	0.61 - 0.74	 1.24A	 38D	 26	 7	 27
	0.97 - 1.07	 21.8A	 29D	 27	 12	 31
	1.27 - 1.37	 21.8A	 28D	 28	 10	 33
	1.42 - 1.52	 14.4A	 31D	 27	 10	 33
	1.6 - 1.68	 27.9A	 33D	 29	 10	 27
	2.06 - 2.13	 23.7A	 28D	 29	 10	 32
	2.69 - 2.79	 33A	 30D	 28	 9	 32
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.2 - 0.3
	0.36 - 0.46
	0.61 - 0.74
	0.97 - 1.07
	1.27 - 1.37
	1.42 - 1.52
	1.6 - 1.68
	2.06 - 2.13
	2.69 - 2.79

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C141	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance