Project Name:	CAN
	Project Code:	CAN	Site ID:	C4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	D.C. van Dijk	Locality:	County Cooper Parish Dallas boundary 1702-1703 
	160M w homestead
	Date Desc.:	01/10/53	Elevation:	 150 metres
	Map Ref.:	Sheet No. : 8128   1:100000	Rainfall:	410
	Northing/Long.:	146.216666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-34.6	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Trampled, Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Subnatric Red Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Sod grass, , . *Species includes - None recorded
	Tall Strata - Tree, , Isolated plants. *Species includes - None Recorded
	Surface Coarse Fragments:	2-10%, , , Quartz
	Profile Morphology
	A11	0 - 0.04 m	Reddish brown (5YR4/4-Moist); ; Fine sandy medium clay; Weak grade of structure, 10-20 mm, 
	Angular blocky; Moderately moist; Weak consistence; Field pH 6.6 (pH meter); Gradual change 
	to - 
	A12	0.04 - 0.11 m	Yellowish red (5YR4/5-Moist); ; Fine sandy medium clay; Weak grade of structure, 5-10 mm, 
	Angular blocky; Moist; Weak consistence; Field pH 6.9 (pH meter); Gradual change to - 
	A13	0.11 - 0.15 m	Reddish brown (5YR4/4-Moist); ; Clay loam; Massive grade of structure; Moist; Firm 
	consistence; Field pH 7.1 (pH meter); Sharp change to - 
	B11	0.15 - 0.24 m	Reddish brown (2.5YR4/4-Moist); ; Heavy clay (Light); Moderate grade of structure, 100-200 mm, 
	Prismatic; Moist; Firm consistence; Field pH 7.8 (pH meter); Gradual change to - 
	B12	0.24 - 0.38 m	Reddish brown (2.5YR4/4-Moist); ; Heavy clay (Light); Weak grade of structure, 50-100 mm, 
	Angular blocky; Moist; Firm consistence; Few (2 - 10 %), Calcareous, , Soft segregations; , 
	Gypseous, Medium (2 -6 mm), Crystals; Field pH 8.9 (pH meter); Sharp change to - 
	B21	0.38 - 0.61 m	Yellowish red (5YR4/6-Moist); ; Heavy clay (Light); Weak grade of structure, 50-100 mm, Angular
	 blocky; Moist; Firm consistence; Common (10 - 20 %), Calcareous, , Soft segregations; , 
	Gypseous, Coarse (6 - 20 mm), Crystals; Field pH 9.1 (pH meter); Gradual change to - 
	C11	0.81 - 0.97 m	Yellowish red (5YR5/8-Moist); ; Medium clay (Heavy); Moderately moist; Firm consistence; 
	Common (10 - 20 %), Calcareous, , Soft segregations; , Gypseous, Medium (2 -6 mm), Crystals; 
	Field pH 8.6 (pH meter); Sharp change to - 
	D1	1.52 - 1.68 m	Pale red (2.5YR6/2-Moist); ; Light clay (Heavy); Moderately moist; Very firm consistence; Field 
	pH 9 (pH meter); 
	Morphological Notes
	Observation Notes
	WIDGELLI LAND SURFACE BEELBANGERA CLAY LOAM                                                                             
	Site Notes

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	WHITTON YANCO

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	6.6A	 0.02C	 5.9K	 1.6	 1.1	 0.12	 4.8E	 13.5B
	0.04 - 0.11	6.9A	 0.014C	 4.7K	 2.3	 0.76	 0.26	 3.6E	 11.6B
	0.11 - 0.15	7.1A	 0.016C	 26.2B
	0.15 - 0.24	7.8A	 0.033C	 11.9K	 10.7	 0.85	 2.7
	0.24 - 0.38	8.9A	 0.11C
	0.38 - 0.61	9.1A	 0.19C
	0.81 - 0.97	8.6A	 0.43C
	1.52 - 1.68	9A	 0.15C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 0.02D	 0.158B	 26D	 42	 9	 21
	0.04 - 0.11	 0.016D	 0.082B	 19D	 43	 18	 18
	0.11 - 0.15	 0.062B	 18D	 41	 19	 19
	0.15 - 0.24	<0.01A	 9D	 21	 7	 59
	0.24 - 0.38	 1.1A	 7D	 18	 6	 65
	0.38 - 0.61	 5.9A
	0.81 - 0.97	 4.9A	 7D	 22	 9	 54
	1.52 - 1.68	 0.21A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.11
	0.11 - 0.15
	0.15 - 0.24
	0.24 - 0.38
	0.38 - 0.61
	0.81 - 0.97
	1.52 - 1.68

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance