Project Name:	CAN
	Project Code:	CAN	Site ID:	C406	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	Adjacent to Narram Coolambund Lagoon:Darlington 
	Pt.
	Date Desc.:	09/11/59	Elevation:	 140 metres
	Map Ref.:	Sheet No. : 8028   1:100000	Rainfall:	410
	Northing/Long.:	145.994444444445	Runoff:	Slow
	Easting/Lat.:	-34.5252777777778	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Porous, Sand 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Orthic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Siliceous sand
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Sod grass, , . *Species includes - Danthonia species
	Tall Strata - Tree, , . *Species includes - Pinus species
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.03 m	Brown (10YR5/3-Dry); ; Loamy sand; Massive grade of structure; Sandy (grains prominent) fabric;
	 Very weak consistence; Field pH 6.6 (pH meter); Diffuse change to - 
	0.03 - 0.15 m	Light brown (7.5YR6/4-Dry); ; Sand; Massive grade of structure; Sandy (grains prominent) fabric; 
	Very weak consistence; 2-10%, fine gravelly, 2-6mm, Shells, coarse fragments; Field pH 6.2 (pH
	 meter); Diffuse change to - 
	0.15 - 0.36 m	Strong brown (7.5YR3/5-Dry); ; Sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Very weak consistence; Field pH 5.5 (pH meter); Few, coarse (>5mm) roots; Gradual 
	change to - 
	0.41 - 0.61 m	Brown (7.5YR4/4-Dry); , 7.5YR56; Sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Very weak consistence; Field pH 6.7 (pH meter); 
	0.71 - 0.91 m	Strong brown (7.5YR5/6-Moist); ; Sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Very weak consistence; Field pH 7.4 (pH meter); 
	1.02 - 1.22 m	Strong brown (7.5YR5/6-Moist); ; Sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Very weak consistence; Field pH 7.4 (pH meter); 
	1.47 - 1.57 m	Reddish yellow (7.5YR6/6-Moist); ; Sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Loose consistence; Field pH 8.6 (pH meter); Sharp change to - 
	1.57 - 1.73 m	Reddish yellow (7.5YR6/6-Moist); , 10YR74; Sandy medium clay; Massive grade of structure; 
	Loose consistence; Many (20 - 50 %), Argillaceous, Coarse (6 - 20 mm), Laminae; Field pH 8.9 
	(pH meter); 
	2.13 - 2.29 m	Brownish yellow (10YR6/6-Moist); ; Sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Loose consistence; Field pH 8.2 (pH meter); 
	3.35 - 3.51 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Loose consistence; Field pH 7.9 (pH meter); 
	Morphological Notes
	Observation Notes

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C406	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	RIVER SAND BLOWN INTO HILLS ADJACENT TO PRIOR STREAM COURSE: 157-173CM BANDS OF CLAY 7.5CM APART 
	~1CM IN THICKNESS      
	Site Notes
	RIVERINA

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C406	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	6.6A	 0.06A	 4.2K	 0.8	 0.4	 0.01	 2.2E	 7.6B
	0.03 - 0.15	6.2A	 0.03A	 2.1K	 0.31	 0.16	 0	 2.2E	 4.8B
	0.15 - 0.36	5.5A	<0.03A	 0.81K	 0.3	 0.1	 0.01	 2.4E	 3.6B
	0.41 - 0.61	6.7A	<0.03A	 1.5K	 0.5	 0.16	 0	 1.1E	 3.3B
	0.71 - 0.91	7.4A	<0.03A	 1.8K	 0.35	 0.14	 0.05	 0.53E	 2.9B
	1.02 - 1.22	7.4A	<0.03A
	1.47 - 1.57	8.6A	 0.06A	 1.6K	 0.22	 0.08	 0.04	 1.9B
	1.57 - 1.73	8.9A	 0.06A	 2.3K	 0.25	 0.08	 0.01	 2.6B
	2.13 - 2.29	8.2A	 0.03A
	3.35 - 3.51	7.9A	 0.03A	 1.3K	 0.3	 0.06	 0.04	 0.24E	 1.9B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 1.2F	 0.023D	 0.111B	 50D	 37	 6	 6
	0.03 - 0.15	 0.34F	 0.019D	 0.032B	 61D	 29	 5	 7
	0.15 - 0.36	 0.24F	 0.019D	 0.012B	 57D	 32	 6	 5
	0.41 - 0.61	 58D	 32	 8	 4
	0.71 - 0.91	 41D	 37	 16	 9
	1.02 - 1.22
	1.47 - 1.57	 0.06A
	1.57 - 1.73	 0.06A	 39D	 38	 16	 9
	2.13 - 2.29	 0.01A
	3.35 - 3.51	 0.01A	 69D	 20	 6	 3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.15
	0.15 - 0.36
	0.41 - 0.61
	0.71 - 0.91
	1.02 - 1.22
	1.47 - 1.57
	1.57 - 1.73
	2.13 - 2.29
	3.35 - 3.51

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C406	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance