Project Name:	CAN
	Project Code:	CAN	Site ID:	C550	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	Tubbo site 16A-AM
	Date Desc.:	01/12/61	Elevation:	 150 metres
	Map Ref.:	Sheet No. : 8128   1:100000	Rainfall:	410
	Northing/Long.:	146.034444444444	Runoff:	Very slow
	Easting/Lat.:	-34.6666666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	<1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Hypocalcic Brown Chromosol     	Principal Profile Form:	Db1.1
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:	Low Strata - Forb, <0.25m, Closed or dense. *Species includes - None recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	0 - 0.1 m	Greyish brown (10YR5/2-Dry); , 10YR62, 20-50% ; , 20-50% ; Clay loam; , Subangular blocky; 
	Massive grade of structure; Medium, (5 - 10) mm crack; Firm consistence; Field pH 6.4 (pH 
	meter); 
	0.1 - 0.3 m	Brown (7.5YR4/3-Dry); ; Medium heavy clay; 50-100 mm, Angular blocky; Medium, (5 - 10) mm 
	crack; Very firm consistence; Field pH 8.1 (pH meter); 
	0.3 - 1.07 m	Brown (7.5YR4/4-Moist); , 7.5YR56, 20-50% ; , 20-50% ; Medium heavy clay; , Angular blocky; 
	Massive grade of structure; Fine, (0 - 5) mm crack; Very firm consistence; Very few (0 - 2 %), 
	Calcareous, , Concretions; 
	1.07 - 1.27 m	Brown (7.5YR4/4-Moist); , 7.5YR56; , 5Y62; Medium heavy clay; Weak consistence; 
	Morphological Notes
	Observation Notes
	BLACK SPECKLING 107-127CM                                                                                               
	Site Notes
	COLEAMBALLY

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C550	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.025	5.9A	 0.12A
	0.025 - 0.1	6.5A	 0.06A	 9K	 8.8	 0.87	 0.8	 6.8E	 26.3B
	0.1 - 0.2
	0.2 - 0.3	8.1A	 0.12A	 15K	 15.2	 1.1	 2.6	 3.4E	 37.3B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.025	 13D	 34	 16	 36
	0.025 - 0.1	 0.7F	 9D	 24	 19	 45
	0.1 - 0.2
	0.2 - 0.3	 0.02A	 5D	 14	 7	 71
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.025
	0.025 - 0.1
	0.1 - 0.2
	0.2 - 0.3

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C550	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance