Project Name:	CAN
	Project Code:	CAN	Site ID:	C555	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	Tubbo site 17B-VM
	Date Desc.:	01/12/61	Elevation:	 150 metres
	Map Ref.:	Sheet No. : 8128   1:100000	Rainfall:	410
	Northing/Long.:	146.034444444444	Runoff:	Very slow
	Easting/Lat.:	-34.6666666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	<1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm, Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Hypocalcic Red Chromosol     	Principal Profile Form:	Dr1.13
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:	Low Strata - Forb, <0.25m, Closed or dense. *Species includes - None recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	0 - 0.13 m	Pale brown (10YR6/3-Dry); , 7.5YR33; , 10YR72; Loam; , Subangular blocky; Massive grade of 
	structure; Firm consistence; Field pH 6.1 (pH meter); 
	0.13 - 0.2 m	Dark reddish brown (5YR3/4-Dry); ; Medium heavy clay; , Angular blocky; Massive grade of 
	structure; Medium, (5 - 10) mm crack; Very firm consistence; Very few (0 - 2 %), Calcareous, , 
	Concretions; 
	0.2 - 0.6 m	Yellowish red (5YR4/5-Dry); ; Medium heavy clay; , Angular blocky; Massive grade of structure; 
	Fine, (0 - 5) mm crack; Very firm consistence; Very few (0 - 2 %), Calcareous, , Concretions; 
	Field pH 7.9 (pH meter); 
	0.6 - 1.07 m	Brown (7.5YR4/4-Moist); ; Medium heavy clay; , Angular blocky; Massive grade of structure; Fine,
	 (0 - 5) mm crack; Very firm consistence; Very few (0 - 2 %), Calcareous, , Concretions; 
	1.07 - 1.27 m	Brown (7.5YR4/4-Moist); , 5Y62; Medium heavy clay; , Angular blocky; Massive grade of 
	structure; Weak consistence; 
	Morphological Notes
	Observation Notes
	BLACK SPECKLING 107-127CM                                                                                               
	Site Notes
	COLEAMBALLY

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C555	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.025	5.8A	 0.15A	 4.7K	 2.7	 0.59	 0.17	 5E	 13.2B
	0.025 - 0.1	6.2A	 0.03A	 3.7K	 3	 0.39	 0.32	 3.9E	 11.3B
	0.1 - 0.2
	0.2 - 0.3	7.9A	 0.15A	 13.4K	 15.8	 0.75	 3	 2.4E	 35.4B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.025	 0.83F	1.51	 14D	 40	 24	 22
	0.025 - 0.1	 0.52F	1.62	 14D	 39	 27	 22
	0.1 - 0.2	1.41
	0.2 - 0.3	 0.04A	1.33	 6D	 17	 9	 68
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.025	15.2H	6.1D
	0.025 - 0.1	15.7H	5.9D
	0.1 - 0.2
	0.2 - 0.3	34.1H	22.7D

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C555	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P3A1_CLOD	Bulk density  g/cm3 - Clods at 0.1 Bar moisture content (McIntyre & Stirk, 1954, Aust. J. Agric. Res. 
	5:291-6)
	P3B1GV_15	15 BAR Moisture g/g - Gravimetric of ground sample (<2mm) using pressure plate
	P3B5GV_01	0.1 BAR Moisture g/g - Gravimetric of soil clods (CSIRO Div. Of Soils TM 25/66)