Project Name:	CAN
	Project Code:	CAN	Site ID:	C560	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	Tubbo site 18B-AM
	Date Desc.:	01/12/61	Elevation:	 150 metres
	Map Ref.:	Sheet No. : 8128   1:100000	Rainfall:	410
	Northing/Long.:	146.033333333333	Runoff:	Very slow
	Easting/Lat.:	-34.7666666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	<1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Surface crust, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Calcic Red Chromosol     	Principal Profile Form:	Dr1.13
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:	Low Strata - Forb, <0.25m, Closed or dense. *Species includes - None recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	0 - 0.1 m	Brown (7.5YR5/4-Dry); ; Clay loam; 20-50 mm, Subangular blocky; Massive grade of structure; 
	Medium, (5 - 10) mm crack; Firm consistence; Field pH 5.8 (pH meter); Wavy change to - 
	0.1 - 0.25 m	Dark reddish brown (5YR3/4-Dry); ; Medium heavy clay; 20-50 mm, Angular blocky; Massive 
	grade of structure; Fine, (0 - 5) mm crack; Very firm consistence; 
	0.25 - 0.76 m	Dark reddish brown (5YR3/4-Dry); ; Medium heavy clay; 20-50 mm, Angular blocky; Massive 
	grade of structure; Fine, (0 - 5) mm crack; Very firm consistence; Few (2 - 10 %), Calcareous, , 
	Concretions; Field pH 8.2 (pH meter); 
	0.76 - 1.27 m	Brown (7.5YR4/3-Moist); , 7.5YR55, 20-50% ; , 20-50% ; Medium heavy clay; 10-20 mm, Angular 
	blocky; Fine, (0 - 5) mm crack; Weak consistence; Very few (0 - 2 %), Calcareous, , Concretions;
	 Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; 
	Morphological Notes
	Observation Notes
	BLACK STAINING:OLIVE GREY MOTTLING AND SHINY PED FACES 76-127CM                                                         
	Site Notes
	COLEAMBALLY

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C560	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.025	5.4A	 0.18A
	0.025 - 0.1	5.9A	 0.06A	 4.1K	 2.7	 0.65	 0.15	 5.7E	 13.3B
	0.1 - 0.2
	0.2 - 0.3	8.2A	 0.15A	 14.2K	 17.3	 1.4	 3.6	 2E	 38.5B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.025	 21D	 42	 20	 17
	0.025 - 0.1	 0.82F	 19D	 42	 18	 18
	0.1 - 0.2
	0.2 - 0.3	 0.02A	 7D	 17	 7	 65
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.025
	0.025 - 0.1
	0.1 - 0.2
	0.2 - 0.3

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C560	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance