Project Name:	CAN
	Project Code:	CAN	Site ID:	C562	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	Tubbo site 19A-AM
	Date Desc.:	01/12/61	Elevation:	 150 metres
	Map Ref.:	Sheet No. : 8128   1:100000	Rainfall:	410
	Northing/Long.:	146.033333333333	Runoff:	Very slow
	Easting/Lat.:	-34.7	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	<1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm, Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Calcic Red Chromosol     	Principal Profile Form:	Dr1.13
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:	Low Strata - Forb, <0.25m, Closed or dense. *Species includes - None recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	0 - 0.12 m	Greyish brown (10YR5/2-Dry); , 10YR53, 20-50% ; , 20-50% ; Sandy clay loam; Massive grade of 
	structure; Firm consistence; Field pH 5.7 (pH meter); 
	0.12 - 0.3 m	Reddish brown (5YR4/3-Dry); , 5YR33, 20-50% ; , 20-50% ; Medium heavy clay; 5-10 mm, 
	Angular blocky; Strong grade of structure, 200-500 mm, Prismatic; Firm consistence; Very few 
	(0 - 2 %), Calcareous, , Concretions; Field pH 8.2 (pH meter); 
	0.3 - 0.76 m	Yellowish red (5YR4/6-Dry); ; Medium heavy clay; 20-50 mm, Angular blocky; Firm consistence; 
	Common (10 - 20 %), Calcareous, , Concretions; Few (2 - 10 %), Gypseous, Fine (0 - 2 mm), 
	Crystals; 
	0.76 - 1.07 m	Brown (10YR5/3-Moist); , 2.5Y52; Medium heavy clay; 20-50 mm, Angular blocky; Firm 
	consistence; Few (2 - 10 %), Calcareous, , Concretions; Few (2 - 10 %), Gypseous, Fine (0 - 2 
	mm), Crystals; 
	1.07 - 1.27 m	Olive grey (5Y5/2-Moist); ; Medium heavy clay; 20-50 mm, Angular blocky; Firm consistence; 
	Morphological Notes
	Observation Notes
	GUN METAL MOTTLING 10-12CM                                                                                              
	Site Notes
	COLEAMBALLY

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C562	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.025	5.6A	 0.09A	 4.7K	 1.1	 0.45	 0.18	 5.5E	 11.9B
	0.025 - 0.1	5.8A	 0.03A	 4.2K	 1.1	 0.49	 0.08	 4.5E	 10.4B
	0.1 - 0.2
	0.2 - 0.3	8.2A	 0.27A	 14.9K	 10.7	 0.98	 3.1	 1.2E	 30.9B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.025	 0.68F	 31D	 30	 17	 13
	0.025 - 0.1	 0.48F	 33D	 39	 16	 11
	0.1 - 0.2
	0.2 - 0.3	 0.02A	 15D	 18	 7	 58
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.025
	0.025 - 0.1
	0.1 - 0.2
	0.2 - 0.3

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C562	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance