Project Name:	CAN
	Project Code:	CAN	Site ID:	CP113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	C.L. Watson	Locality:	~7KM east of Bellata:Terry Hie Hie Road
	Date Desc.:	30/08/78	Elevation:	 280 metres
	Map Ref.:	Sheet No. : 8838   1:100000	Rainfall:	640
	Northing/Long.:	149.883333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-29.9	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Rolling low hills 30-90m 10-	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	1 % 	Aspect:	300 degrees
	Surface Soil Condition (dry):	Recently cultivated, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Self-Mulching Black Vertosol     	Principal Profile Form:	Ug5.14
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); ; Light medium clay; 2-5 mm, Granular; Very weak 
	consistence; Moderately plastic; Non-sticky; Common (10 - 20 %), Calcareous, , Soft 
	segregations; Field pH 8.4 (pH meter); 
	0.05 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); ; Medium heavy clay; Massive grade of structure; Weak
	 consistence; Slightly plastic; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 
	8.4 (pH meter); 
	0.1 - 0.2 m	Very dark greyish brown (10YR3/2-Moist); ; Medium heavy clay; Massive grade of structure; Weak
	 consistence; Slightly plastic; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 
	8.5 (pH meter); 
	0.2 - 0.3 m	Very dark greyish brown (10YR3/2-Moist); ; Medium heavy clay; Massive grade of structure; Weak
	 consistence; Slightly plastic; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 
	8.6 (pH meter); 
	0.3 - 0.4 m	Very dark greyish brown (10YR3/2-Moist); ; Medium heavy clay; Weak consistence; Slightly 
	plastic; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 8.7 (pH meter); 
	0.4 - 0.5 m	Very dark greyish brown (10YR3/2-Moist); ; Medium heavy clay; Weak consistence; Slightly 
	plastic; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 8.8 (pH meter); 
	0.5 - 0.6 m	Very dark greyish brown (10YR3/2-Moist); ; Medium heavy clay; Weak consistence; Slightly 
	plastic; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 8.9 (pH meter); 
	0.6 - 0.7 m	Very dark greyish brown (10YR3/2-Moist); ; Medium heavy clay; Weak consistence; Slightly 
	plastic; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 8.9 (pH meter); 
	0.7 - 0.8 m	Dark grey (10YR4/1-Moist); , 10YR63, 20-50% ; , 20-50% ; Medium heavy clay; Weak 
	consistence; Slightly plastic; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 9 
	(pH meter); 
	0.8 - 1 m	Very pale brown (10YR7/3-Moist); ; Medium heavy clay; Very weak consistence; Common (10 - 
	20 %), Calcareous, , Soft segregations; Calcrete; Field pH 9.1 (pH meter); 
	Morphological Notes
	Observation Notes

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Notes
	BELLATA
	CARBONATE CEMENTED LAYER 100CM                                                                                          

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	8.4A	 0.13A	 42.3K	 16.8	 1.2	 0.52	 4.9B	 65.8J	0.79
	0.05 - 0.1	8.5A	 0.13A
	0.1 - 0.2	8.6A	 0.15A
	0.2 - 0.3	8.7A	 0.18A
	0.3 - 0.4	8.8A	 0.19A
	0.4 - 0.5	8.9A	 0.21A
	0.5 - 0.6	8.9A	 0.25A
	0.6 - 0.7	9A	 0.26A
	0.7 - 0.8	9.1A	 0.27A
	0.8 - 1	9.2A	 0.29A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 2.57A	 1.05D	 6D	 22	 12	 53
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05	 0.27B
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 1

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP113	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate