Project Name:	CAN
	Project Code:	CAN	Site ID:	CP117	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	C.L. Watson	Locality:	~6KM East of Cryon along Burren Junction Road then
	 turn off to Rayleigh
	Date Desc.:	02/09/78	Elevation:	 160 metres
	Map Ref.:	Sheet No. : 8637   1:100000	Rainfall:	500
	Northing/Long.:	148.683333333333	Runoff:	Very slow
	Easting/Lat.:	-30.0333333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Episodic-Epicalcareous Self-Mulching Brown Vertosol     	Principal Profile Form:	Ug5.34
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark brown (10YR3/3-Moist); , 10YR43, 20-50% ; , 20-50% ; Medium clay; Weak grade of 
	structure, 5-10 mm, Angular blocky; Very weak consistence; Moderately plastic; Slightly sticky; 
	Many (20 - 50 %), Calcareous, , Soft segregations; Field pH 8.2 (pH meter); 
	0.1 - 0.2 m	Dark brown (10YR3/3-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Angular 
	blocky; Weak consistence; Many (20 - 50 %), Calcareous, , Soft segregations; Field pH 8.7 (pH 
	meter); 
	0.2 - 0.3 m	Dark brown (10YR3/3-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Angular 
	blocky; Firm consistence; Many (20 - 50 %), Calcareous, , Soft segregations; Field pH 8.9 (pH 
	meter); 
	0.3 - 0.4 m	Dark brown (10YR3/3-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Angular 
	blocky; Firm consistence; Many (20 - 50 %), Calcareous, , Soft segregations; Field pH 9 (pH 
	meter); 
	0.4 - 0.5 m	Dark brown (10YR3/3-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Angular 
	blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Concretions; Field pH 9 (pH meter); 
	0.5 - 0.6 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	20-50 mm, Angular blocky; Firm consistence; Many (20 - 50 %), Calcareous, , Soft segregations;
	 Field pH 9 (pH meter); 
	0.6 - 0.7 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	20-50 mm, Angular blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Concretions; Field 
	pH 8.9 (pH meter); 
	0.7 - 0.8 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	20-50 mm, Angular blocky; Firm consistence; Many (20 - 50 %), Calcareous, , Soft segregations;
	 Field pH 8.8 (pH meter); 
	0.8 - 0.9 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	5-10 mm; Firm consistence; Few (2 - 10 %), Calcareous, , Concretions; Few (2 - 10 %), 
	Gypseous, Fine (0 - 2 mm), Crystals; Field pH 7.9 (pH meter); 

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP117	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	0.9 - 1 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	5-10 mm; Firm consistence; Many (20 - 50 %), Calcareous, , Soft segregations; Few (2 - 10 %), 
	Gypseous, Fine (0 - 2 mm), Crystals; Field pH 7.8 (pH meter); 
	1 - 1.1 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	5-10 mm, Angular blocky; Firm consistence; Many (20 - 50 %), Calcareous, , Soft segregations; 
	Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field pH 8.1 (pH meter); 
	1.1 - 1.2 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	5-10 mm, Angular blocky; Firm consistence; Many (20 - 50 %), Calcareous, , Soft segregations; 
	Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field pH 8.1 (pH meter); 
	1.2 - 1.3 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	5-10 mm, Angular blocky; Firm consistence; Many (20 - 50 %), Calcareous, , Soft segregations; 
	Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field pH 7.9 (pH meter); 
	1.3 - 1.4 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	5-10 mm, Angular blocky; Firm consistence; Many (20 - 50 %), Calcareous, , Soft segregations; 
	Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field pH 8 (pH meter); 
	1.4 - 1.5 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	10-20 mm, Angular blocky; Very firm consistence; Few (2 - 10 %), Calcareous, , Concretions; 
	Field pH 8.4 (pH meter); 
	1.5 - 1.6 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	10-20 mm, Angular blocky; Very firm consistence; Many (20 - 50 %), Calcareous, , Soft 
	segregations; Field pH 8.3 (pH meter); 
	1.6 - 1.7 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	10-20 mm, Angular blocky; Very firm consistence; Few (2 - 10 %), Calcareous, , Concretions; 
	Field pH 8.4 (pH meter); 
	1.7 - 1.8 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	10-20 mm, Angular blocky; Very firm consistence; Many (20 - 50 %), Calcareous, , Soft 
	segregations; Field pH 8.2 (pH meter); 
	1.8 - 1.9 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	10-20 mm, Angular blocky; Very firm consistence; Few (2 - 10 %), Calcareous, , Concretions; 
	Field pH 8.4 (pH meter); 
	1.9 - 2 m	Brown (10YR4/3-Moist); , 10YR53, 20-50% ; , 20-50% ; Medium clay; Strong grade of structure, 
	10-20 mm, Angular blocky; Very firm consistence; Many (20 - 50 %), Calcareous, , Soft 
	segregations; Field pH 8.1 (pH meter); 
	Morphological Notes
	Observation Notes
	140-200CM BLACK STAINING ON FACES                                                                                       
	Site Notes
	CRYON

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP117	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.2A	 0.12A	 8.7K	 4	 2.5	 1.6	 4.3B	 21.1J	7.58
	0.1 - 0.2	8.7A	 0.25A
	0.2 - 0.3	8.9A	 0.26A
	0.3 - 0.4	9A	 0.28A
	0.4 - 0.5	9A	 0.35A
	0.5 - 0.6	9A	 0.47A
	0.6 - 0.7	8.9A	 0.68A
	0.7 - 0.8	8.8A	 0.88A
	0.8 - 0.9	7.9A	 2.9A
	0.9 - 1	7.8A	 3.5A
	1 - 1.1	8.1A	 2.4A
	1.1 - 1.2	8.1A	 2.5A
	1.2 - 1.3	7.9A	 2.7A
	1.3 - 1.4	8A	 2.3A
	1.4 - 1.5	8.4A	 1.7A
	1.5 - 1.6	8.3A	 1.6A
	1.6 - 1.7	8.4A	 1.5A
	1.7 - 1.8	8.2A	 1.5A
	1.8 - 1.9	8.4A	 1.5A
	1.9 - 2	8.1A	 1.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.05A	 1.04D	 19D	 26	 24	 29
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	1 - 1.1
	1.1 - 1.2
	1.2 - 1.3
	1.3 - 1.4
	1.4 - 1.5
	1.5 - 1.6
	1.6 - 1.7
	1.7 - 1.8
	1.8 - 1.9
	1.9 - 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	 0.13B

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP117	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	1 - 1.1
	1.1 - 1.2
	1.2 - 1.3
	1.3 - 1.4
	1.4 - 1.5
	1.5 - 1.6
	1.6 - 1.7
	1.7 - 1.8
	1.8 - 1.9
	1.9 - 2

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP117	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate