Project Name:	CAN
	Project Code:	CAN	Site ID:	CP120	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	C.L. Watson	Locality:	College Green 5KM from last Walgett turn off:Cryon 
	Road:
	Date Desc.:	03/09/78	Elevation:	 1 metres
	Map Ref.:	Sheet No. : 8538   1:100000	Rainfall:	480
	Northing/Long.:	148.25	Runoff:	Very slow
	Easting/Lat.:	-29.9666666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Episodic-Epicalcareous Self-Mulching Grey Vertosol     	Principal Profile Form:	Ug5.24
	ASC Confidence:	Great Soil Group:	Grey clay
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:	Low Strata - Sod grass, , . *Species includes - Triticum aestivum
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.03 m	Dark greyish brown (10YR4/2-Moist); , 10YR52, 20-50% ; , 20-50% ; Heavy clay; Strong grade of 
	structure, <2 mm, Granular; Very weak consistence; Moderately plastic; Moderately sticky; 
	0.03 - 0.1 m	Dark greyish brown (10YR4/2-Moist); , 10YR52, 20-50% ; , 20-50% ; Heavy clay; Strong grade of 
	structure, 20-50 mm, Angular blocky; Very weak consistence; Moderately plastic; Moderately 
	sticky; Field pH 8.5 (pH meter); 
	0.1 - 0.2 m	Dark greyish brown (10YR4/2-Moist); , 10YR52, 20-50% ; , 20-50% ; Heavy clay; Massive grade of
	 structure; Very weak consistence; Moderately plastic; Moderately sticky; Field pH 8.7 (pH 
	meter); 
	0.2 - 0.3 m	Dark greyish brown (10YR4/2-Moist); , 10YR52, 20-50% ; , 20-50% ; Heavy clay; Massive grade of
	 structure; Very weak consistence; Moderately plastic; Moderately sticky; Few (2 - 10 %), 
	Calcareous, , Concretions; Field pH 8.7 (pH meter); 
	0.3 - 0.4 m	Dark greyish brown (10YR4/2-Moist); , 10YR52, 20-50% ; , 20-50% ; Heavy clay; Massive grade of
	 structure; Very weak consistence; Moderately plastic; Moderately sticky; Few (2 - 10 %), 
	Calcareous, , Concretions; Field pH 9 (pH meter); 
	0.4 - 0.5 m	Dark greyish brown (10YR4/2-Moist); , 10YR52, 20-50% ; , 20-50% ; Heavy clay; Massive grade of
	 structure; Very weak consistence; Moderately plastic; Moderately sticky; Few (2 - 10 %), 
	Calcareous, , Concretions; Field pH 8.9 (pH meter); 
	0.5 - 0.6 m	Dark greyish brown (10YR4/2-Moist); , 10YR52, 20-50% ; , 20-50% ; Heavy clay; Massive grade of
	 structure; Very weak consistence; Moderately plastic; Moderately sticky; Few (2 - 10 %), 
	Calcareous, , Concretions; Field pH 8.7 (pH meter); 
	0.6 - 0.7 m	Dark greyish brown (10YR4/2-Moist); , 10YR52, 20-50% ; , 20-50% ; Heavy clay; Massive grade of
	 structure; Very weak consistence; Moderately plastic; Moderately sticky; Few (2 - 10 %), 
	Calcareous, , Concretions; Field pH 8.5 (pH meter); 
	0.7 - 0.8 m	Dark greyish brown (10YR4/2-Moist); , 10YR52, 20-50% ; , 20-50% ; Heavy clay; Massive grade of
	 structure; Very weak consistence; Moderately plastic; Moderately sticky; Few (2 - 10 %), 
	Calcareous, , Concretions; Field pH 7.7 (pH meter); 

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP120	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	0.8 - 0.9 m	Brown (10YR5/3-Moist); ; Heavy clay; Massive grade of structure; Weak consistence; Moderately 
	plastic; Slightly sticky; Common (10 - 20 %), Calcareous, , Soft segregations; Very few (0 - 2 %),
	 Gypseous, Fine (0 - 2 mm), Crystals; Field pH 7.6 (pH meter); 
	0.9 - 1 m	Brown (10YR5/3-Moist); ; Heavy clay; Massive grade of structure; Few (<1 per 100mm2) Fine (1-
	2mm) macropores, Very weak consistence; Slightly plastic; Slightly sticky; Common (10 - 20 %),
	 Calcareous, , Concretions; Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field pH 7.6
	 (pH meter); 
	1 - 1.1 m	Brown (10YR5/3-Moist); ; Heavy clay; Massive grade of structure; Few (<1 per 100mm2) Fine (1-
	2mm) macropores, Very weak consistence; Slightly plastic; Slightly sticky; Common (10 - 20 %),
	 Calcareous, , Soft segregations; Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field 
	pH 7.6 (pH meter); 
	1.1 - 1.2 m	Brown (10YR5/3-Moist); ; Heavy clay; Massive grade of structure; Few (<1 per 100mm2) Fine (1-
	2mm) macropores, Very weak consistence; Slightly plastic; Slightly sticky; Common (10 - 20 %),
	 Calcareous, , Concretions; Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field pH 7.6
	 (pH meter); 
	1.2 - 1.3 m	Brown (10YR5/3-Moist); ; Heavy clay; Massive grade of structure; Few (<1 per 100mm2) Fine (1-
	2mm) macropores, Very weak consistence; Slightly plastic; Slightly sticky; Common (10 - 20 %),
	 Calcareous, , Soft segregations; Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field 
	pH 7.7 (pH meter); 
	1.3 - 1.4 m	Brown (10YR5/3-Moist); ; Heavy clay; Massive grade of structure; Few (<1 per 100mm2) Fine (1-
	2mm) macropores, Very weak consistence; Slightly plastic; Slightly sticky; Common (10 - 20 %),
	 Calcareous, , Concretions; Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field pH 7.9
	 (pH meter); 
	1.4 - 1.5 m	Brown (10YR5/3-Moist); ; Heavy clay; Massive grade of structure; Few (<1 per 100mm2) Fine (1-
	2mm) macropores, Weak consistence; Common (10 - 20 %), Calcareous, , Soft segregations; 
	Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field pH 8 (pH meter); 
	1.5 - 1.6 m	Brown (10YR5/3-Moist); ; Heavy clay; Massive grade of structure; Few (<1 per 0.01m2) Medium 
	(2-5mm) macropores, Weak consistence; Many (20 - 50 %), Calcareous, , Concretions; Very few 
	(0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field pH 7.9 (pH meter); 
	1.6 - 1.7 m	Brown (10YR5/3-Moist); ; Heavy clay; Massive grade of structure; Few (<1 per 0.01m2) Medium 
	(2-5mm) macropores, Weak consistence; Many (20 - 50 %), Calcareous, , Soft segregations; 
	Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field pH 8.4 (pH meter); 
	1.7 - 1.8 m	Brown (10YR5/3-Moist); ; Heavy clay; Massive grade of structure; Few (<1 per 0.01m2) Medium 
	(2-5mm) macropores, Weak consistence; Many (20 - 50 %), Calcareous, , Concretions; Very few 
	(0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field pH 8.4 (pH meter); 
	1.8 - 1.9 m	Brown (10YR5/3-Moist); ; Heavy clay; Weak grade of structure, 10-20 mm, Angular blocky; Few 
	(<1 per 0.01m2) Medium (2-5mm) macropores, Very firm consistence; Many (20 - 50 %), 
	Calcareous, , Soft segregations; Field pH 8.5 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	WALGETT

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP120	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	8.5A	 0.15A	 24.7K	 9.7	 1.4	 1.8	 4.4B	 42J	4.29
	0.03 - 0.1	8.7A	 0.14A
	0.1 - 0.2	8.7A	 0.24A
	0.2 - 0.3	9A	 0.23A
	0.3 - 0.4	8.9A	 0.32A
	0.4 - 0.5	8.7A	 0.45A
	0.5 - 0.6	8.5A	 0.78A
	0.6 - 0.7	7.7A	 2.2A
	0.7 - 0.8	7.6A	 3.4A
	0.8 - 0.9	7.6A	 3.8A
	0.9 - 1	7.6A	 4.1A
	1 - 1.1	7.6A	 4.4A
	1.1 - 1.2	7.7A	 4.3A
	1.2 - 1.3	7.9A	 3.1A
	1.3 - 1.4	8A	 2.9A
	1.4 - 1.5	7.9A	 2.8A
	1.5 - 1.6	8.4A	 1.7A
	1.6 - 1.7	8.4A	 1.7A
	1.7 - 1.8	8.5A	 1.5A
	1.8 - 1.9	8.5A	 1.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 0.27A	 0.61D	 6D	 21	 16	 55
	0.03 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	1 - 1.1
	1.1 - 1.2
	1.2 - 1.3
	1.3 - 1.4
	1.4 - 1.5
	1.5 - 1.6
	1.6 - 1.7
	1.7 - 1.8
	1.8 - 1.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03	 0.21B

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP120	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	0.03 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	1 - 1.1
	1.1 - 1.2
	1.2 - 1.3
	1.3 - 1.4
	1.4 - 1.5
	1.5 - 1.6
	1.6 - 1.7
	1.7 - 1.8
	1.8 - 1.9

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP120	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate