Project Name:	CAN
	Project Code:	CAN	Site ID:	CP144	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	G.A. Stewart	Locality:	Over Gin Gin Bridge Macquarie River before culvert 
	Trangie Road
	Date Desc.:	09/06/79	Elevation:	 225 metres
	Map Ref.:	Sheet No. : SH8534   1:10000	Rainfall:	500
	Northing/Long.:	148.083333333333	Runoff:	Very slow
	Easting/Lat.:	-31.9333333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	280 degrees
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous-Endohypersodic Self-Mulching Brown Vertosol	Principal Profile Form:	Ug5.34
	     
	ASC Confidence:	Great Soil Group:	Grey clay
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark brown (7.5YR3/4-Moist); ; Medium heavy clay; Moderate grade of structure, 2-5 mm, Angular
	 blocky; Very coarse, (20 - 50) mm crack; Very weak consistence; Moderately plastic; Slightly 
	sticky; Many (20 - 50 %), Calcareous, , Soft segregations; Field pH 8.3 (pH meter); 
	0.1 - 0.2 m	Dark brown (7.5YR3/4-Moist); ; Medium heavy clay; Moderate grade of structure, 2-5 mm, Angular
	 blocky; Coarse, (10 - 20) mm crack; Very weak consistence; Moderately plastic; Slightly sticky; 
	Many (20 - 50 %), Calcareous, , Concretions; Field pH 8.4 (pH meter); 
	0.2 - 0.3 m	Dark brown (7.5YR3/4-Moist); ; Medium heavy clay; Moderate grade of structure, 2-5 mm, Angular
	 blocky; Very weak consistence; Moderately plastic; Slightly sticky; 2-10%, fine gravelly, 2-6mm, 
	rounded, dispersed, Quartz, coarse fragments; Many (20 - 50 %), Calcareous, , Soft 
	segregations; Field pH 8.6 (pH meter); Sharp change to - 
	0.3 - 0.4 m	Reddish brown (5YR4/3-Moist); ; Medium heavy clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Very firm consistence; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, 
	coarse fragments; Many (20 - 50 %), Calcareous, , Concretions; Field pH 8.7 (pH meter); 
	0.4 - 0.5 m	Reddish brown (5YR4/3-Moist); ; Medium heavy clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Very firm consistence; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, 
	coarse fragments; Many (20 - 50 %), Calcareous, , Soft segregations; Field pH 8.8 (pH meter); 
	0.5 - 0.6 m	Reddish brown (5YR4/3-Moist); ; Medium heavy clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Very firm consistence; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, 
	coarse fragments; Many (20 - 50 %), Calcareous, , Concretions; Field pH 8.9 (pH meter); 
	0.6 - 0.7 m	Reddish brown (5YR4/3-Moist); ; Medium heavy clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Very firm consistence; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, 
	coarse fragments; Many (20 - 50 %), Calcareous, , Soft segregations; Field pH 8.9 (pH meter); 
	0.7 - 0.8 m	Reddish brown (5YR4/3-Moist); ; Medium heavy clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Very firm consistence; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, 
	coarse fragments; Many (20 - 50 %), Calcareous, , Concretions; Field pH 8.8 (pH meter); 
	0.8 - 0.9 m	Reddish brown (5YR4/3-Moist); ; Medium heavy clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Very firm consistence; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, 
	coarse fragments; Many (20 - 50 %), Calcareous, , Soft segregations; Field pH 8.7 (pH meter); 

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP144	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	0.9 - 1 m	Reddish brown (5YR4/3-Moist); ; Medium heavy clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Very firm consistence; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, 
	coarse fragments; Many (20 - 50 %), Calcareous, , Concretions; Field pH 8.1 (pH meter); 
	1 - 1.1 m	Reddish brown (5YR4/3-Moist); ; Medium heavy clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Very firm consistence; Many (20 - 50 %), Calcareous, , Concretions; Field pH 
	7.8 (pH meter); 
	1.1 - 1.2 m	Reddish brown (5YR4/4-Moist); , 5YR43, 2-10% ; , 2-10% ; Medium heavy clay; Weak grade of 
	structure, 2-5 mm, Angular blocky; Firm consistence; Many (20 - 50 %), Calcareous, , Soft 
	segregations; Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Crystals; Field pH 7.6 (pH meter); 
	1.2 - 1.3 m	Reddish brown (5YR4/4-Moist); ; Medium heavy clay; Weak grade of structure, 2-5 mm, Angular 
	blocky; Firm consistence; Many (20 - 50 %), Calcareous, , Soft segregations; Very few (0 - 2 %), 
	Gypseous, Fine (0 - 2 mm), Crystals; Field pH 7.7 (pH meter); 
	1.3 - 1.4 m	Yellowish red (5YR4/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Very few (0 - 2 %), 
	Gypseous, Fine (0 - 2 mm), Crystals; Field pH 8.1 (pH meter); 
	1.4 - 1.5 m	Yellowish red (5YR4/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Field pH 8 (pH 
	meter); 
	1.5 - 1.6 m	Yellowish red (5YR4/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Field pH 7.1 (pH 
	meter); 
	1.6 - 1.7 m	Yellowish red (5YR4/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Field pH 6.3 (pH 
	meter); 
	1.7 - 1.8 m	Yellowish red (5YR4/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Field pH 5.6 (pH 
	meter); 
	1.8 - 1.9 m	Yellowish red (5YR4/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Field pH 5.3 (pH 
	meter); 
	1.9 - 2 m	Yellowish red (5YR4/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Field pH 5.2 (pH 
	meter); 
	Morphological Notes
	Observation Notes
	SHINY SURFACES >30CM                                                                                                    
	Site Notes
	TRANGIE

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP144	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.3A	 0.12C	 23.5K	 4.3	 1.1	 0.3	 5.6B	 34.8J	0.86
	0.1 - 0.2	8.4A	 0.13C
	0.2 - 0.3	8.6A	 0.16C
	0.3 - 0.4	8.7A	 0.22C
	0.4 - 0.5	8.8A	 0.26C
	0.5 - 0.6	8.9A	 0.33C
	0.6 - 0.7	8.9A	 0.39C
	0.7 - 0.8	8.8A	 0.49C
	0.8 - 0.9	8.7A	 0.61C
	0.9 - 1	8.1A	 1.55C
	1 - 1.1	7.8A	 2.4C
	1.1 - 1.2	7.6A	 2.9C
	1.2 - 1.3	7.7A	 2.5C
	1.3 - 1.4	8.1A	 1.03C
	1.4 - 1.5	8A	 0.92C
	1.5 - 1.6	7.1A	 0.89C
	1.6 - 1.7	6.3A	 0.92C
	1.7 - 1.8	5.6A	 0.91C
	1.8 - 1.9	5.3A	 0.87C
	1.9 - 2	5.2A	 0.84C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 2.07A	 1.09D	 8D	 34	 9	 43
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	1 - 1.1
	1.1 - 1.2
	1.2 - 1.3
	1.3 - 1.4
	1.4 - 1.5
	1.5 - 1.6
	1.6 - 1.7
	1.7 - 1.8
	1.8 - 1.9
	1.9 - 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	 0.17B

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP144	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	1 - 1.1
	1.1 - 1.2
	1.2 - 1.3
	1.3 - 1.4
	1.4 - 1.5
	1.5 - 1.6
	1.6 - 1.7
	1.7 - 1.8
	1.8 - 1.9
	1.9 - 2

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP144	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate