Project Name:	CAN
	Project Code:	CAN	Site ID:	CP159	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	P.H. Walker	Locality:	Flood behind levee CP 158
	Date Desc.:	01/01/79	Elevation:	 12 metres
	Map Ref.:	Sheet No. : 9030   	Rainfall:	800
	Northing/Long.:	150.7225	Runoff:	Slow
	Easting/Lat.:	-33.5966666666667	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Soil pit, Porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Flood plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic Eutrophic Red Kandosol     	Principal Profile Form:	Gn2.11
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Tall Strata - Tree, 3.01-6m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.15 m	Dark brown (7.5YR3/2-Moist); ; Loamy sand; Massive grade of structure; Weak consistence; 
	Clear change to - 
	11A	0.15 - 0.3 m	Dark reddish brown (5YR3/2-Moist); ; Sandy loam (Light); Massive grade of structure; Weak 
	consistence; Field pH 6.2 (pH meter); 
	A	0.3 - 0.45 m	Dark reddish brown (5YR3/2-Moist); ; Sandy loam; Massive grade of structure; Weak 
	consistence; Gradual change to - 
	B1	0.45 - 0.67 m	Dark reddish brown (5YR3/3-Moist); ; Sandy loam (Heavy); Massive grade of structure; Very 
	strong consistence; Field pH 6.2 (pH meter); Gradual change to - 
	B21	0.67 - 0.88 m	Reddish brown (5YR4/4-Moist); ; Clay loam; Massive grade of structure; Very strong 
	consistence; Field pH 6.2 (pH meter); Gradual change to - 
	B22	0.88 - 1.1 m	Yellowish red (5YR4/6-Moist); ; Clay loam; Massive grade of structure; Very strong consistence; 
	B31	1.1 - 1.3 m	Yellowish red (5YR4/6-Moist); ; Sandy loam; Massive grade of structure; Very strong 
	consistence; Field pH 6.4 (pH meter); 
	B32	1.3 - 1.5 m	Yellowish red (5YR4/6-Moist); ; Sandy loam; Massive grade of structure; Very strong 
	consistence; 
	C1	1.5 - 1.7 m	Yellowish red (5YR4/6-Moist); ; Sandy loam; Massive grade of structure; Very firm consistence; 
	Field pH 6.5 (pH meter); 
	Morphological Notes
	Observation Notes
	MODERN/HOLOCENE ALLUVIUM:45-88CM SL.VESICULAR:0-15 LATE FLOOD DEPOSIT:                                                  
	Site Notes
	RICHMOND

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP159	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.15 - 0.3	6.2A	 0.02A	 4.7K	 1.2	 0.09	 0	 6.7B	 12.7J	0.00
	0.45 - 0.67	6.2A	 0.02A	 4.4K	 1.3	 0.1	 0.07	 4.2B	 10.1J	0.69
	0.67 - 0.88	6.2A	 0.02A	 3.5K	 1.4	 0.11	 0.07	 6B	 11.1J	0.63
	1.1 - 1.3	6.4A	 0.02A	 2.7K	 1.6	 0.1	 0.04	 3.2B	 7.6J	0.53
	1.5 - 1.7	6.5A	 0.02A	 1.9K	 1.2	 0.06	 0	 1.8B	 5J	0.00
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.15 - 0.3	 1.07D	 3D	 60	 21	 15
	0.45 - 0.67	 0.62D	 8D	 44	 25	 23
	0.67 - 0.88	 0.5D	 9D	 45	 23	 24
	1.1 - 1.3	 0.21D	 17D	 46	 17	 21
	1.5 - 1.7	 0.12D	 32D	 44	 11	 13
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.15 - 0.3
	0.45 - 0.67
	0.67 - 0.88
	1.1 - 1.3
	1.5 - 1.7

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP159	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	13_C_FE	Extractable Fe(%) - Method recorded as C
	13A1_AL	Oxalate-extractable aluminium
	13A1_FE	Oxalate-extractable iron
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance