Project Name:	CAN
	Project Code:	CAN	Site ID:	CP163	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	D. McGarry	Locality:	Garoka paddock 8 east end
	Date Desc.:	20/11/79	Elevation:	 200 metres
	Map Ref.:	Sheet No. : 8737   1:100000	Rainfall:	640
	Northing/Long.:	149.201944444444	Runoff:	Very slow
	Easting/Lat.:	-30.1538888888889	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching, Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Episodic-Epicalcareous Self-Mulching Grey Vertosol     	Principal Profile Form:	Ug5.15
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:
	Tall Strata - Forb, 1.01-3m, Closed or dense. *Species includes - None Recorded
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, , Quartz
	Profile Morphology
	0 - 0.1 m	Very dark grey (10YR3/1-Moist); , 10YR32; Medium heavy clay; Strong grade of structure, 5-10 
	mm, Subangular blocky; Loose consistence; 0-2%, fine gravelly, 2-6mm, dispersed, Quartz, 
	coarse fragments; Field pH 7.8 (pH meter); Clear change to - 
	0.1 - 0.2 m	Very dark grey (10YR3/1-Moist); , 10YR32; Medium heavy clay; 10-20 mm, Subangular blocky; 
	Firm consistence; Field pH 8.4 (pH meter); Clear change to - 
	0.2 - 0.3 m	Very dark grey (10YR3/1-Moist); , 10YR32; Medium heavy clay; Strong grade of structure, 20-50 
	mm, Angular blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Concretions; Field pH 8.8 
	(pH meter); Diffuse, Tongued change to - 
	0.3 - 0.4 m	Brown (10YR4/3-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, Angular 
	blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Concretions; Field pH 8.9 (pH meter); 
	Morphological Notes
	Observation Notes
	LAND PLANED:SEDIMENTS OF BASALTIC (MAJOR) AND SEDIMENTARY ORIGIN                                                        
	Site Notes
	MERAH NORTH

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP163	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.8A	 0.22A	 22K	 13.2	 1.3	 2.1	 8.4B	 47J	4.47
	0.1 - 0.2	7.9A	 0.19A	 21.5K	 13	 1	 2.9	 7B	 45.4J	6.39
	0.2 - 0.3	8.5A	 0.13A	 20.4K	 13.6	 0.89	 4.5	 6.9B	 46.2J	9.74
	0.3 - 0.4	8.7A	 0.2A	 19.2K	 13.6	 0.86	 6.3	 6.2B	 46.2J	13.64
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.17A	 2.13D	 41A	 0.102B	 5D	 11	 20	 59
	0.1 - 0.2	 1.05D	 32.6A	 0.083B
	0.2 - 0.3	 0.74D	 16.8A
	0.3 - 0.4	 0.41A	 0.7D	 16.4A	 5D	 10	 22	 62
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP163	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance