Project Name:	GH
	Project Code:	GH	Site ID:	CP2	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	Woolsides cotton area
	Date Desc.:	01/10/68	Elevation:	 120 metres
	Map Ref.:	Sheet No. : 8029   1:100000	Rainfall:	400
	Northing/Long.:	145.9	Runoff:	Very slow
	Easting/Lat.:	-34.3833333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Recently cultivated
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epihypersodic-Endocalcareous Epipedal Red Vertosol     	Principal Profile Form:	Ug5.38
	ASC Confidence:	Great Soil Group:	Red clay
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Brown (7.5YR4/2-Moist); ; Medium clay; 10-20 mm, Angular blocky; Very firm consistence; Few 
	(2 - 10 %), Calcareous, , Concretions; Field pH 7.8 (pH meter); 
	0.1 - 0.2 m	Dark reddish brown (5YR3/3-Moist); ; Heavy clay; 10-20 mm, Angular blocky; Very firm 
	consistence; 
	0.2 - 0.3 m	Reddish brown (5YR4/3-Moist); ; Heavy clay; 10-20 mm, Angular blocky; Very firm consistence; 
	Field pH 8.3 (pH meter); 
	0.3 - 0.4 m	Reddish brown (5YR4/3-Moist); ; Heavy clay; 10-20 mm, Angular blocky; Very firm consistence; 
	0.4 - 0.5 m	Reddish brown (5YR4/4-Moist); ; Heavy clay; 10-20 mm, Angular blocky; Very firm consistence; 
	Field pH 8.9 (pH meter); 
	0.5 - 0.6 m	Reddish brown (5YR4/4-Moist); ; Heavy clay; 10-20 mm, Angular blocky; Very firm consistence; 
	Few (2 - 10 %), Calcareous, , Concretions; 
	0.6 - 0.7 m	Yellowish red (5YR4/5-Moist); ; Heavy clay; 10-20 mm, Angular blocky; Very firm consistence; 
	Few (2 - 10 %), Calcareous, , Concretions; Field pH 9.1 (pH meter); 
	0.7 - 0.8 m	Yellowish red (5YR4/5-Moist); , 7.5YR54, 20-50% ; , 20-50% ; Medium clay; 10-20 mm, Angular 
	blocky; Weak consistence; Very few (0 - 2 %), Calcareous, , Concretions; 
	0.8 - 0.9 m	Light yellowish brown (10YR6/4-Moist); , 7.5YR42; , 5YR56; Medium clay; 10-20 mm, Angular 
	blocky; Weak consistence; Very few (0 - 2 %), Calcareous, , Concretions; Field pH 8.9 (pH 
	meter); 
	0.9 - 1 m	Light yellowish brown (10YR6/4-Moist); , 7.5YR54; , 5YR56; Medium clay; 10-20 mm, Angular 
	blocky; Weak consistence; Very few (0 - 2 %), Calcareous, , Concretions; 
	Morphological Notes
	Observation Notes
	ALLUVIUM                                                                                                                
	Site Notes
	BEHEREMBAH

	Project Name:	GH
	Project Code:	GH	Site ID:	CP2	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)

	Project Name:	GH
	Project Code:	GH	Site ID:	CP2	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.8A	 0.16A	 14.2K	 5.7	 1.9	 1	1.9D	 25.4J	3.94
	7.8A	0.15A	15.4K	7	2.1	0.79	27.2J	2.90
	0 - 0.1	7.8A	 0.16A	 14.2K	 5.7	 1.9	 1	1.9D	 25.4J	3.94
	7.8A	0.15A	15.4K	7	2.1	0.79	27.2J	2.90
	0.1 - 0.2	 1.9
	0.2 - 0.3	8.3A	 0.13A	 11.9K	 13.1	 1.3	 3.4	 34.7J	9.80
	0.4 - 0.5	8.9A	 0.25A
	0.6 - 0.7	9.1A	 0.47A
	0.8 - 0.9	8.9A	 0.81A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.05A	 1.12D	 58A	 12D	 33	 8	 44
	1.1D	69A	11D	33	10	46
	0 - 0.1	 0.05A	 1.12D	 58A	 12D	 33	 8	 44
	1.1D	69A	11D	33	10	46
	0.1 - 0.2
	0.2 - 0.3	 0.07A	 3A
	0.4 - 0.5	 2A
	0.6 - 0.7	 3A
	0.8 - 0.9	 2A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.4 - 0.5
	0.6 - 0.7
	0.8 - 0.9

	Project Name:	GH
	Project Code:	GH	Site ID:	CP2	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance