Project Name:	GH
	Project Code:	GH	Site ID:	CP27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	22KM N.W. along Deniliquin/Hay Road
	Date Desc.:	31/10/68	Elevation:	 120 metres
	Map Ref.:	Sheet No. : 7827   1:100000	Rainfall:	420
	Northing/Long.:	144.866666666667	Runoff:	Very slow
	Easting/Lat.:	-35.3833333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	<1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Cracking, Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Vertic Mesonatric Grey Sodosol     	Principal Profile Form:	Ug5.5
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Sod grass, , . *Species includes - None recorded
	Mid Strata - Chenopod shrub, , . *Species includes - Atriplex vesicaria
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Clay loam; Massive grade of structure; Medium, (5 - 10) 
	mm crack; Very weak consistence; Field pH 5.7 (pH meter); Sharp change to - 
	0.05 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Medium heavy clay; Weak grade of structure, 20-50 mm, 
	Angular blocky; Medium, (5 - 10) mm crack; Weak consistence; Field pH 6.4 (pH meter); 
	0.1 - 0.2 m	Dark greyish brown (10YR4/2-Moist); ; Medium heavy clay; Weak grade of structure, 20-50 mm, 
	Angular blocky; Weak consistence; 
	0.2 - 0.3 m	Dark greyish brown (10YR4/2-Moist); ; Medium heavy clay; Moderate grade of structure, 100-200 
	mm, Angular blocky; Weak consistence; Field pH 7 (pH meter); 
	0.3 - 0.4 m	Dark greyish brown (10YR4/2-Moist); ; Medium heavy clay; Weak consistence; Few (2 - 10 %), 
	Calcareous, , Soft segregations; 
	0.4 - 0.5 m	Dark greyish brown (10YR4/2-Moist); ; Medium heavy clay; Weak consistence; Few (2 - 10 %), 
	Calcareous, , Soft segregations; Field pH 6.8 (pH meter); 
	0.5 - 0.6 m	Dark greyish brown (10YR4/2-Moist); ; Medium heavy clay; Weak consistence; Few (2 - 10 %), 
	Calcareous, , Soft segregations; 
	0.6 - 0.7 m	Brown (10YR5/3-Moist); ; Medium heavy clay; Weak consistence; Few (2 - 10 %), Calcareous, , 
	Soft segregations; Field pH 6.8 (pH meter); 
	0.7 - 0.8 m	Brown (10YR5/3-Moist); ; Medium heavy clay; Weak consistence; Few (2 - 10 %), Calcareous, , 
	Soft segregations; 
	0.8 - 0.9 m	Brown (10YR5/3-Moist); ; Medium heavy clay; Weak consistence; Few (2 - 10 %), Calcareous, , 
	Concretions; Few (2 - 10 %), Gypseous, , ; Field pH 6.9 (pH meter); 
	Morphological Notes
	Observation Notes
	ALLUVIUM BILLABONG CLAY LAYERS RE NUMBERED 21/10/92                                                                     
	Site Notes
	DENILIQUIN

	Project Name:	GH
	Project Code:	GH	Site ID:	CP27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)

	Project Name:	GH
	Project Code:	GH	Site ID:	CP27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.7A	 0.15A	 3.7K	 5.1	 0.98	 0.78	 18.5J	4.22
	0 - 0.1	7.2A	0.06A	7.8K	11.6	1.1	3.3	5.3D	29.1J	11.34
	0.05 - 0.1	6.4A	 0.31A	 8.1K	 11.6	 1.2	 3	 31.4J	9.55
	0.2 - 0.3	7A	 1.87A	 9.2K	 15.2	 0.98	 6.5	 36J	18.06
	0.4 - 0.5	6.8A	 3.13A
	0.6 - 0.7	6.8A	 2.78A
	0.8 - 0.9	6.9A	 5.85A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0A	 1.54D	 15A	 11D	 39	 15	 32
	0 - 0.1	1.1D	8.5A	8D	25	10	57
	0.05 - 0.1	 0A	 0.76D	 7A	 5D	 21	 13	 59
	0.2 - 0.3	 0A	 5A
	0.4 - 0.5	 0A	 4A
	0.6 - 0.7	 0A	 3A
	0.8 - 0.9	 0A	 4A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0 - 0.1
	0.05 - 0.1
	0.2 - 0.3
	0.4 - 0.5
	0.6 - 0.7
	0.8 - 0.9

	Project Name:	GH
	Project Code:	GH	Site ID:	CP27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance