Project Name:	LSG
	Project Code:	LSG	Site ID:	CP65	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	P.H. Walker	Locality:	Gauging Station (ford) high alluvial bench
	Date Desc.:	01/07/76	Elevation:	 680 metres
	Map Ref.:	Sheet No. : 8727   1:100000	Rainfall:	640
	Northing/Long.:	149.266666666667	Runoff:	Slow
	Easting/Lat.:	-35.1833333333334	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	1.5 m deep,Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Terrace (alluvial)
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	125 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic Regolithic Chernic Tenosol     	Principal Profile Form:	Uc
	ASC Confidence:	Great Soil Group:	Alluvial soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Sod grass, , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Massive grade of structure; Very weak 
	consistence; Field pH 6.4 (pH meter); 
	0.1 - 0.22 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Massive grade of structure; Very weak 
	consistence; Field pH 6.4 (pH meter); Abrupt change to - 
	0.22 - 0.4 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy loam; Massive grade of structure; Firm 
	consistence; Field pH 6.2 (pH meter); Diffuse change to - 
	0.4 - 0.45 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Massive grade of structure; Very weak 
	consistence; Field pH 6.3 (pH meter); Abrupt change to - 
	0.45 - 0.48 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy loam; Massive grade of structure; Very firm 
	consistence; Field pH 6.3 (pH meter); Abrupt change to - 
	0.48 - 0.55 m	Dark greyish brown (10YR4/2-Moist); ; Fine sandy loam; Massive grade of structure; Very firm 
	consistence; Field pH 6.3 (pH meter); Abrupt change to - 
	0.55 - 0.69 m	Dark greyish brown (10YR4/2-Moist); ; Fine sandy loam; Massive grade of structure; Very firm 
	consistence; Field pH 6.3 (pH meter); Abrupt change to - 
	AB	0.69 - 0.85 m	Very dark greyish brown (10YR3/2-Moist); ; Fine sandy loam; Massive grade of structure; Very 
	firm consistence; Field pH 6.1 (pH meter); Abrupt change to - 
	AB	0.85 - 1.1 m	Very dark greyish brown (10YR3/2-Moist); ; Fine sandy loam; Massive grade of structure; Very 
	firm consistence; Field pH 6.5 (pH meter); Diffuse change to - 
	B	1.1 - 1.3 m	Black (2.5Y2/2-Moist); , 7.5YR44, 2-10% ; , 2-10% ; Clay loam, fine sandy; Moderate grade of 
	structure, 20-50 mm, Angular blocky; Very firm consistence; Common cutans, 10-50% of ped 
	faces or walls coated, distinct; Field pH 7.5 (pH meter); Diffuse change to - 
	B	1.3 - 1.35 m	Dark greyish brown (2.5Y4/2-Moist); , 10YR55, 2-10% ; , 2-10% ; Sandy clay loam; Massive grade
	 of structure; Very firm consistence; Field pH 7.7 (pH meter); 
	CB	1.35 - 1.4 m	Dark greyish brown (2.5Y4/2-Moist); , 10YR55, 2-10% ; , 2-10% ; Sandy clay loam; Massive grade
	 of structure; Very firm consistence; Field pH 7.7 (pH meter); 

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP65	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	CB	1.4 - 1.45 m	Dark greyish brown (2.5Y4/2-Moist); , 10YR55, 2-10% ; , 2-10% ; Sandy clay loam; Massive grade
	 of structure; Very firm consistence; Field pH 7.7 (pH meter); 
	CB	1.45 - 1.5 m	Dark greyish brown (2.5Y4/2-Moist); , 10YR55, 2-10% ; , 2-10% ; Sandy clay loam; Massive grade
	 of structure; Very firm consistence; Field pH 7.3 (pH meter); 
	Morphological Notes
	Observation Notes
	ALLUVIUM  0-40CM FAUNAL CHANNELS TO 2CM DIAMETER 45-69 SEDT. LAMINATED ZONE    69-110 BIOTURBATED       
	                
	Site Notes
	UPPER YASS RV.

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP65	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.5A	<0.04A	 2.5K	 2.1	 0.29	 0.02	 2.7B	 9J	0.22
	0.05 - 0.1	6.4A	<0.04A	 2.8K	 1.9	 0.15	 0.03	 5.1B	 10J	0.30
	0.1 - 0.15	6.3A	<0.04A	 3.3K	 2.1	 0.08	 0.04	 5B	 10.5J	0.38
	0.15 - 0.2	6.5A	<0.04A	 3K	 2.1	 0.08	 0.04	 2.8B	 8J	0.50
	0.2 - 0.22	6.4A	<0.04A	 2.6K	 1.9	 0.07	 0.05	 2.9B	 7.5J	0.67
	0.22 - 0.25	6.4A	<0.04A	 3.2K	 2.4	 0.09	 0.08	 3.7B	 9.5J	0.84
	0.25 - 0.3	6.2A	<0.04A	 3.7K	 2.7	 0.08	 0.11	 7.4B	 14J	0.79
	0.3 - 0.35	6A	<0.04A	 3.2K	 2.5	 0.06	 0.11	 7.1B	 13J	0.85
	0.35 - 0.4	6.1A	<0.04A	 3.5K	 2.5	 0.08	 0.15	 7.3B	 13.5J	1.11
	0.4 - 0.45	6.3A	<0.04A	 2.5K	 1.9	 0	 0.05	 6B	 10.5J	0.48
	0.45 - 0.48	6.3A	<0.04A	 3.3K	 2.2	 0.03	 0.15	 8.8B	 14.5J	1.03
	0.48 - 0.5	6.3A	<0.04A	 2.8K	 2	 0.08	 0.24	 4.4B	 9.5J	2.53
	0.5 - 0.55	6.3A	<0.04A	 3.2K	 2.2	 0.07	 0.25	 8.3B	 14J	1.79
	0.55 - 0.6	6.3A	<0.04A	 3.6K	 2.2	 0.07	 0.27	 6.9B	 13J	2.08
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.9D	 0.086B
	0.05 - 0.1	 0.79D	 0.066B
	0.1 - 0.15	 0.8D	 0.071B
	0.15 - 0.2	 0.8D	 0.072B
	0.2 - 0.22	 0.72D	 0.066B
	0.22 - 0.25	 0.92D	 0.069B
	0.25 - 0.3	 1.39D	 0.086B
	0.3 - 0.35	 1.66D	 0.071B
	0.35 - 0.4	 0.99D	 0.077B
	0.4 - 0.45	 0.72D	 0.053B
	0.45 - 0.48	 0.96D	 0.062B
	0.48 - 0.5	 0.6D	 0.05B
	0.5 - 0.55	 0.89D	 0.065B
	0.55 - 0.6	 0.83D	 0.064B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.22
	0.22 - 0.25
	0.25 - 0.3
	0.3 - 0.35
	0.35 - 0.4
	0.4 - 0.45
	0.45 - 0.48
	0.48 - 0.5
	0.5 - 0.55

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP65	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	0.55 - 0.6

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP65	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded