Project Name:	MUR
	Project Code:	MUR	Site ID:	C129	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	H.M. Churchwood	Locality:	1.2km S fo N bdry, 2km W of E bndry portion 16 
	parish of Bynuce.
	Date Desc.:	26/10/56	Elevation:	 61 metres
	Map Ref.:	Rainfall:	305
	Northing/Long.:	Runoff:	Moderately rapid
	Easting/Lat.:	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Dunefield
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Swale	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red-brown earth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	Ap	0 - 0.1 m	Yellowish red (5YR4/6-Moist); ; Loamy sand; Weak grade of structure, 20-50 mm, Angular 
	blocky; Weak grade of structure, 10-20 mm, Angular blocky; 
	A	0.15 - 0.2 m	Red (2.5YR4/8-Moist); ; Loamy sand; Massive grade of structure; Abrupt change to - 
	B1	0.23 - 0.3 m	Red (2.5YR4/6-Moist); , 2.5YR58; Sandy medium clay; Weak grade of structure, 20-50 mm, 
	Angular blocky; Clear change to - 
	Bk	0.33 - 0.41 m	Red (2.5YR4/6-Moist); , 2.5YR68; , 5YR46; Fine sandy medium clay; Weak grade of structure, 5-
	10 mm, Angular blocky; Few (2 - 10 %), Calcareous, , Soft segregations; 
	0.41 - 0.48 m	Red (2.5YR4/6-Moist); , 2.5YR68; , 5YR46; Medium clay; Moderate grade of structure, 10-20 mm,
	 Angular blocky; Few (2 - 10 %), Calcareous, , Soft segregations; Clear change to - 
	0.53 - 0.61 m	Red (2.5YR4/8-Moist); , 5YR54; , 5YR68; Sandy medium clay; Moderate grade of structure, 20-
	50 mm, Angular blocky; 
	0.61 - 0.76 m	Red (2.5YR4/8-Moist); , 5YR58; , 2.5YR68; Sandy medium clay; Moderate grade of structure, 10-
	20 mm, Angular blocky; Many (20 - 50 %), Calcareous, Coarse (6 - 20 mm), Concretions; 
	0.94 - 1.12 m	Red (2.5YR4/8-Moist); , 2.5Y84; Sandy clay loam; Massive grade of structure; Many (20 - 50 %), 
	Calcareous, Medium (2 -6 mm), Concretions; Clear change to - 
	1.3 - 1.42 m	Red (10R4/8-Moist); ; Fine sandy medium clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; Common (10 - 20 %), Calcareous, Medium (2 -6 mm), Concretions; 
	2.24 - 2.49 m	Red (10R4/6-Moist); , 10YR73; , 10YR63; Fine sandy medium clay (Heavy); Moderate grade of 
	structure, 10-20 mm, Angular blocky; 
	Morphological Notes
	Observation Notes
	SEE ORIGIAL PROFILE DESCRIPTION FOR MORE DETIAL:                                                                        
	Site Notes
	MURRAKOOL

	Project Name:	MUR
	Project Code:	MUR	Site ID:	C129	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	MUR
	Project Code:	MUR	Site ID:	C129	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile