Project Name:	NC
	Project Code:	NC	Site ID:	C404	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	P.H. Walker	Locality:	Ourimbah/Mangrove Mountain Road 5KM from 
	Ourimbah
	Date Desc.:	12/02/59	Elevation:	 215 metres
	Map Ref.:	Sheet No. : 9131   1:100000	Rainfall:	1250
	Northing/Long.:	151.366666666667	Runoff:	Slow
	Easting/Lat.:	-33.35	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Sandstone 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plateau
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Level
	Slope:	<1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Brown Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Yellow earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Sod grass, , . *Species includes - None recorded
	Tall Strata - Tree, , Closed or dense. *Species includes - None Recorded
	Surface Coarse Fragments:	10-20%, , , Charcoal
	Profile Morphology
	A1	0 - 0.08 m	Dark brown (7.5YR3/2-Moist); Pale brown (10YR6/3-Dry); ; Sandy loam; Massive grade of 
	structure; Sandy (grains prominent) fabric; Moist; Weak consistence; 
	AB	0.08 - 0.18 m	Strong brown (7.5YR5/8-Moist); Brownish yellow (10YR6/6-Dry); , 10YR44, 20-50% ; , 20-50% ; 
	Sandy loam; Massive grade of structure; Sandy (grains prominent) fabric; Moist; Weak 
	consistence; 0-2%, coarse gravelly, 20-60mm, rounded, dispersed, Sandstone, coarse 
	fragments; 
	B	0.18 - 0.38 m	Strong brown (7.5YR5/8-Moist); Brownish yellow (10YR6/8-Dry); ; Sandy clay loam (Light); 
	Massive grade of structure; Sandy (grains prominent) fabric; Moist; Weak consistence; 0-2%, 
	coarse gravelly, 20-60mm, rounded, dispersed, Sandstone, coarse fragments; 
	B	0.38 - 0.61 m	Strong brown (7.5YR5/8-Moist); Brownish yellow (10YR6/8-Dry); ; Sandy clay loam; Massive 
	grade of structure; Sandy (grains prominent) fabric; Moist; Weak consistence; 0-2%, coarse 
	gravelly, 20-60mm, rounded, dispersed, Sandstone, coarse fragments; 
	B	0.61 - 0.89 m	Strong brown (7.5YR5/8-Moist); Brownish yellow (10YR6/8-Dry); ; Sandy clay loam (Heavy); 
	Massive grade of structure; Sandy (grains prominent) fabric; Moist; Weak consistence; 2-10%, 
	coarse gravelly, 20-60mm, rounded, dispersed, Sandstone, coarse fragments; Few cutans, 
	<10% of ped faces or walls coated, distinct; 
	BC	0.89 - 1.14 m	Reddish yellow (7.5YR6/8-Moist); Yellow (10YR7/6-Dry); , 10YR68, 20-50% ; , 20-50% ; Sandy 
	clay loam (Heavy); Massive grade of structure; Moist; Weak consistence; 2-10%, coarse gravelly,
	 20-60mm, rounded, dispersed, Sandstone, coarse fragments; Few cutans, <10% of ped faces 
	or walls coated, distinct; 
	BC	1.14 - 1.32 m	Brownish yellow (10YR6/8-Moist); Yellow (10YR7/8-Dry); ; Sandy light clay (Light); Massive 
	grade of structure; Wet; Weak consistence; 10-20%, cobbly, 60-200mm, rounded, dispersed, 
	Sandstone, coarse fragments; Few cutans, <10% of ped faces or walls coated, distinct; 
	R	1.32 - 1.5 m	Rock 
	Morphological Notes
	R	Parent material:sandstone
	Observation Notes

	Project Name:	NC
	Project Code:	NC	Site ID:	C404	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	TRIASSIC HAWKESBURY SANDSTONE                                                                                           
	Site Notes
	GOSFORD

	Project Name:	NC
	Project Code:	NC	Site ID:	C404	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	NC
	Project Code:	NC	Site ID:	C404	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile