Project Name:	NC
	Project Code:	NC	Site ID:	C454	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	P.H. Walker	Locality:	Corner Yarrahapinni Road and Barbers Lane
	Date Desc.:	06/12/60	Elevation:	 350 metres
	Map Ref.:	Sheet No. : 9436   1:100000	Rainfall:	1200
	Northing/Long.:	152.927777777778	Runoff:	Moderately rapid
	Easting/Lat.:	-30.75	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Steep mountains >300m 32-	Pattern Type:	Mountains
	56%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Mesotrophic Red Dermosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Prairie soil
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Sod grass, , . *Species includes - None recorded
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, angular, Quartz
	Profile Morphology
	A	0 - 0.2 m	Dark brown (7.5YR3/2-Moist); ; Clay loam (Heavy); Massive grade of structure; Moderately moist; 
	Firm consistence; 2-10%, medium gravelly, 6-20mm, angular, dispersed, Quartz, coarse 
	fragments; Field pH 5.8 (pH meter); Many
	A	0.2 - 0.3 m	Dark brown (7.5YR3/3-Moist); ; Light clay (Heavy); Massive grade of structure; Dry; Weak 
	consistence; 2-10%, coarse gravelly, 20-60mm, angular, dispersed, Quartz, coarse fragments; 
	Field pH 5.8 (pH meter); Many
	A	0.3 - 0.43 m	Brown (7.5YR4/2-Moist); , 2.5YR36, 20-50% ; , 20-50% ; Light clay (Heavy); Moderate grade of 
	structure, 10-20 mm, Polyhedral; Moderately moist; Weak consistence; 2-10%, coarse gravelly, 
	20-60mm, angular, dispersed, Quartz, coarse fragments; Field pH 5.4 (pH meter); Common
	B	0.43 - 0.66 m	Dark red (10R3/6-Moist); , 5YR56, 2-10% ; , 2-10% ; Medium clay; Strong grade of structure, 10-
	20 mm, Polyhedral; Moderately moist; Weak consistence; 2-10%, coarse gravelly, 20-60mm, 
	angular, dispersed, Quartz, coarse fragments; Field pH 5.3 (pH meter); Few
	B	0.66 - 1.04 m	Dark red (10R3/6-Moist); ; Heavy clay; Strong grade of structure, 10-20 mm, Subangular blocky; 
	Moist; Very firm consistence; 0-2%, coarse gravelly, 20-60mm, angular, dispersed, Quartz, 
	coarse fragments; Field pH 5 (pH meter); 
	B	1.07 - 1.52 m	Dark red (10R3/6-Moist); , 7.5YR44, 20-50% ; , 20-50% ; Heavy clay; Strong grade of structure, 
	10-20 mm, Angular blocky; Moist; Very firm consistence; 0-2%, angular, dispersed, Quartz, 
	coarse fragments; Very few (0 - 2 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 4.8 
	(pH meter); 
	Morphological Notes
	Observation Notes
	LOBE OF MASS MOVEMENT DETRITUS:WORM FILL TO 70CM                                                                        
	Site Notes
	EUNGAI

	Project Name:	NC
	Project Code:	NC	Site ID:	C454	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.2	5.8A	 0.024A	 1.4K	 0.92	 0.14	 0.21	 13J	1.62
	0.2 - 0.3	5.8A	 0.024A
	0.3 - 0.43	5.4A	 0.03A
	0.43 - 0.66	5.3A	 0.03A	 0.77K	 2.3	 0.2	 0.18	 9.4J	1.91
	0.66 - 1.04	5A	 0.036A
	1.07 - 1.52	4.8A	 0.039A	 0.1K	 1.7	 0.13	 0.16	 8.1J	1.98
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.2	 2.8F	 0.129B	 1	 9D	 19	 39	 30
	0.2 - 0.3	 8	 6D	 17	 34	 41
	0.3 - 0.43	 6	 5D	 15	 29	 48
	0.43 - 0.66	 0.63F	 0.034B	 12	 5D	 12	 20	 61
	0.66 - 1.04
	1.07 - 1.52	 1	 6D	 8	 11	 74
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.2
	0.2 - 0.3
	0.3 - 0.43
	0.43 - 0.66
	0.66 - 1.04
	1.07 - 1.52

	Project Name:	NC
	Project Code:	NC	Site ID:	C454	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	7_NR	Total nitrogen (%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance