Project Name:	SC
	Project Code:	SC	Site ID:	C310	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	P.H. Walker	Locality:	65.6km from Nelligan Point towards Braidwood.
	Date Desc.:	24/01/56	Elevation:	No Data
	Map Ref.:	Sheet No. : 8926   1:100000	Rainfall:	990
	Northing/Long.:	150.166666666667	Runoff:	Rapid
	Easting/Lat.:	-35.6666666666667	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	Steep hills 90-300m 32-56%	Pattern Type:	Hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Steep
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy4.31
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.1 m	Greyish brown (10YR5/2-Moist); ; Clayey sand; Massive grade of structure; Moderately moist; 
	Firm consistence; 10-20%, medium gravelly, 6-20mm, dispersed, Granite, coarse fragments; 
	Gradual change to - 
	A12	0.1 - 0.35 m	Light olive brown (2.5Y5/6-Moist); , 10YR64; , 10YR76; Clayey sand; Massive grade of structure; 
	Weak grade of structure, 5-10 mm, Cast; Dry; Firm consistence; 0-2%, cobbly, 60-200mm, 
	dispersed, Granite, coarse fragments; Gradual change to - 
	A2cb	0.35 - 0.48 m	Light grey (10YR7/2-Moist); , 10YR76; , 10YR56; Clayey sand; Massive grade of structure; Weak 
	grade of structure, 5-10 mm, Cast; Dry; Firm consistence; 0-2%, cobbly, 60-200mm, dispersed, 
	Granite, coarse fragments; Gradual change to - 
	B1	0.48 - 0.68 m	Dark red (2.5YR3/6-Moist); ; Coarse sandy clay loam; Massive grade of structure; Moderately 
	moist; Firm consistence; Gradual change to - 
	BC	0.68 - 0.88 m	Brownish yellow (10YR6/6-Moist); ; Sandy light clay; Massive grade of structure; Moderately 
	moist; Very firm consistence; Common cutans, 10-50% of ped faces or walls coated, distinct; 
	Gradual change to - 
	BC	0.88 - 1.06 m	Brownish yellow (10YR6/6-Moist); ; Sandy light clay; Massive grade of structure; Moderately 
	moist; Very firm consistence; Few cutans, <10% of ped faces or walls coated, distinct; 
	Morphological Notes
	Observation Notes
	FELDSPAR IN B1 HORIZON:                                                                                                 
	Site Notes
	BRAIDWOOD

	Project Name:	SC
	Project Code:	SC	Site ID:	C310	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.9A	<0.03A
	0.1 - 0.35	6.3A	<0.03A
	0.35 - 0.48	6.5A	<0.03A
	0.48 - 0.68	6A	<0.03A
	0.68 - 0.88	5.9A	<0.03A
	0.88 - 1.06	6.3A	<0.03A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.21F	 57D	 27	 9	 6
	0.1 - 0.35	 52D	 30	 11	 9
	0.35 - 0.48	 53D	 28	 12	 9
	0.48 - 0.68	 51D	 21	 7	 19
	0.68 - 0.88	 0.19F	 40D	 24	 8	 25
	0.88 - 1.06	 55D	 23	 5	 18
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.35
	0.35 - 0.48
	0.48 - 0.68
	0.68 - 0.88
	0.88 - 1.06

	Project Name:	SC
	Project Code:	SC	Site ID:	C310	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance