Project Name:	SC
	Project Code:	SC	Site ID:	CP106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	P.H. Walker	Locality:	Mayfair just east of Brunee Swamp:levee toeslope
	Date Desc.:	19/12/78	Elevation:	 1 metres
	Map Ref.:	Sheet No. : 8928   1:100000	Rainfall:	1150
	Northing/Long.:	150.663888888889	Runoff:	Very slow
	Easting/Lat.:	-34.9111111111111	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Flood plain
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Levee	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	No Available Class Stratic Oxyaquic Hydrosol     	Principal Profile Form:	Um5.51
	ASC Confidence:	Great Soil Group:	Alluvial soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Sod grass, <0.25m, Closed or dense. *Species includes - None recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A	0 - 0.1 m	Black (10YR2/1-Moist); ; Loam (Sapric); Massive grade of structure; Moist; Weak consistence; 
	Field pH 4.9 (pH meter); Gradual change to - 
	A	0.1 - 0.15 m	Black (10YR2/1-Moist); ; Loam (Sapric); Massive grade of structure; Moist; Weak consistence; 
	Field pH 4.8 (pH meter); Clear change to - 
	D	0.15 - 0.2 m	Dark grey (5Y4/1-Moist); , 7.5YR44, 2-10% ; , 2-10% ; Medium clay; Weak grade of structure, 20-
	50 mm, Angular blocky; Moist; Firm consistence; Field pH 4.7 (pH meter); Diffuse change to - 
	D	0.2 - 0.3 m	Grey (5Y5/1-Moist); , 10YR44, 0-2% ; , 0-2% ; Sand; Massive grade of structure; Moist; Very weak
	 consistence; Field pH 5 (pH meter); Gradual change to - 
	D	0.3 - 0.4 m	Grey (5Y5/1-Moist); ; Sand; Massive grade of structure; Moist; Loose consistence; Field pH 4.8 
	(pH meter); Gradual change to - 
	D	0.4 - 0.5 m	Grey (5Y5/1-Moist); , 2.5Y53, 2-10% ; , 2-10% ; Loamy sand; Massive grade of structure; Wet; 
	Very weak consistence; Non-plastic; Non-sticky; Field pH 4.5 (pH meter); Gradual change to - 
	D	0.5 - 0.6 m	Grey (5Y5/1-Moist); , 5Y20, 2-10% ; , 7.5YR56, 2-10% ; Sandy loam; Wet; Very weak 
	consistence; Slightly plastic; Slightly sticky; 0-2%, fine gravelly, 2-6mm, rounded, dispersed, 
	Shells, coarse fragments; Very few (0 - 2 %), Ferruginous, Fine (0 - 2 mm), Nodules; Field pH 
	4.7 (pH meter); Gradual change to - 
	D	0.6 - 0.7 m	Grey (5Y5/1-Moist); , 5Y20, 20-50% ; , 20-50% ; Sandy loam; Wet; Very weak consistence; 
	Slightly plastic; Slightly sticky; Field pH 4.6 (pH meter); Gradual change to - 
	D	0.7 - 0.8 m	Grey (5Y5/1-Moist); , 5Y20, 10-20% ; , 10YR66, 10-20% ; Loamy sand; Wet; Very weak 
	consistence; Slightly plastic; Slightly sticky; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, 
	Shells, coarse fragments; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), Tubules; Field pH 4.3
	 (pH meter); Gradual change to - 
	D	0.8 - 0.9 m	Grey (5Y5/1-Moist); , 2.5Y53, 10-20% ; , 10-20% ; Sandy loam; Wet; Very weak consistence; 
	Slightly plastic; Slightly sticky; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 mm), Tubules; Field 
	pH 4.4 (pH meter); Clear change to - 

	Project Name:	SC
	Project Code:	SC	Site ID:	CP106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	D	0.9 - 1 m	Dark grey (5Y4/1-Moist); , 5Y84, 2-10% ; , 2-10% ; Silty loam; Wet; Very weak consistence; 
	Slightly plastic; Slightly sticky; Few (2 - 10 %), Ferruginous, Very coarse (20 - 60 mm), Tubules; 
	Field pH 4.3 (pH meter); Gradual change to - 
	D	1 - 1.3 m	Dark grey (5Y4/1-Moist); , 5Y84, 2-10% ; , 2-10% ; Silty loam; Wet; Very weak consistence; 
	Slightly plastic; Slightly sticky; Field pH 4.4 (pH meter); Gradual change to - 
	D	1.3 - 1.6 m	Very dark grey (2.5Y3/0-Moist); , 10YR44, 0-2% ; , 0-2% ; Silty loam; Wet; Very weak 
	consistence; Moderately plastic; Moderately sticky; Field pH 4.7 (pH meter); Gradual change to - 
	D	1.6 - 1.9 m	Very dark grey (2.5Y3/0-Moist); , 10YR44, 0-2% ; , 0-2% ; Silty loam; Wet; Very weak 
	consistence; Moderately plastic; Moderately sticky; 2-10%, dispersed, Shells, coarse fragments;
	 Field pH 4.9 (pH meter); Gradual change to - 
	D	1.9 - 2 m	Very dark grey (2.5Y3/0-Moist); , 10YR44, 0-2% ; , 0-2% ; Silty loam; Wet; Very weak 
	consistence; Moderately plastic; Moderately sticky; 2-10%, dispersed, Shells, coarse fragments;
	 Field pH 4.9 (pH meter); Gradual change to - 
	Morphological Notes
	Observation Notes
	ALLUVIAL LEVEE SEDIMENTS                                                                                                
	Site Notes
	BRUNDEE

	Project Name:	SC
	Project Code:	SC	Site ID:	CP106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.9A	 0.92A
	0.1 - 0.15	4.8A	 0.71A
	0.15 - 0.2	4.7A	 0.59A
	0.2 - 0.3	5A	 0.24A
	0.3 - 0.4	4.8A	 0.2A
	0.4 - 0.5	4.5A	 0.31A
	0.5 - 0.6	4.7A	 0.4A
	0.6 - 0.7	4.6A	 0.46A
	0.7 - 0.8	4.3A	 0.56A
	0.8 - 0.9	4.4A	 1A
	0.9 - 1	4.3A	 2A
	1 - 1.3	4.4A	 3.1A
	1.3 - 1.6	4.7A	 4.4A
	1.6 - 1.9	4.9A	 4.6A
	1.9 - 2	4.9A	 3.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 19.1D	 5D	 15	 23	 25
	0.1 - 0.15	 10.3D	 3D	 15	 29	 34
	0.15 - 0.2	 5.1D	 2D	 13	 30	 45
	0.2 - 0.3	 0.95D
	0.3 - 0.4	 0.65D	 49D	 36	 10	 7
	0.4 - 0.5	 0.66D
	0.5 - 0.6	 1.44D
	0.6 - 0.7	 1.32D	 8D	 69	 13	 10
	0.7 - 0.8	 0.78D
	0.8 - 0.9	 1.34D
	0.9 - 1	 1.31D
	1 - 1.3	 1.89D	 2D	 49	 27	 20
	1.3 - 1.6	 3.46D
	1.6 - 1.9	 3.52D
	1.9 - 2	 3.94D	 0D	 34	 37	 23
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	SC
	Project Code:	SC	Site ID:	CP106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	1 - 1.3
	1.3 - 1.6
	1.6 - 1.9
	1.9 - 2

	Project Name:	SC
	Project Code:	SC	Site ID:	CP106	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance