Project Name:	WAG
	Project Code:	WAG	Site ID:	C39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	Locality:	Erosion gully north of Henty-Pleasant Hills Road: 
	East of bridge on  Munda Waddery Road 11.3km west
	 of Henty:
	Date Desc.:	11/12/56	Elevation:	 2 metres
	Map Ref.:	Rainfall:	570
	Northing/Long.:	Runoff:	Moderately rapid
	Easting/Lat.:	Drainage:	Moderately well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Pediplain
	Morph. Type:	No Data	Relief:	60 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Ferric Hypercalcic Brown Dermosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Danthonia species
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Light brown (7.5YR6/4-Moist); , 7.5YR58; , 10YR74; Silty clay loam; Weak grade of structure, 50-
	100 mm, Angular blocky; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Firm 
	consistence; 0-2%, Gravel, coarse fragments; Common
	A2	0.1 - 0.18 m	Pink (7.5YR7/4-Moist); , 7.5YR58; , 10YR74; Silty clay loam; Massive grade of structure; Few (<1
	 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Firm consistence; 2-10%, Gravel, coarse 
	fragments; CommonAbrupt change to - 
	AB	0.18 - 0.3 m	Pink (7.5YR7/4-Moist); , 7.5YR56; , 2.5Y62; Silty clay loam; Massive grade of structure; Few (<1 
	per 100mm2) Very fine (0.075-1mm) macropores, Dry; Firm consistence; Wavy change to - 
	B11	0.3 - 0.41 m	Strong brown (7.5YR5/6-Moist); , 2.5Y62; , 5YR56; Medium clay; Strong grade of structure, 5-10 
	mm, Angular blocky; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Moderately moist; Very weak consistence; Few cutans, <10% of ped faces or walls
	 coated; Few (2 - 10 %), Ferruginous, , Concretions; Gradual change to - 
	B12	0.48 - 0.58 m	Brownish yellow (10YR6/6-Moist); , 7.5YR56, 2-10% ; , 5YR56, 2-10% ; Medium heavy clay; 
	Weak grade of structure, 100-200 mm, Prismatic; Moderate grade of structure, <2 mm, Platy; 
	Moderately moist; Weak consistence; 0-2%, Gravel, coarse fragments; Few cutans, <10% of ped
	 faces or walls coated; Very few (0 - 2 %), Ferruginous, Fine (0 - 2 mm), Concretions; Gradual 
	change to - 
	B13	0.71 - 0.84 m	Yellowish brown (10YR5/6-Moist); ; Medium heavy clay; Weak grade of structure, 100-200 mm, 
	Prismatic; 20-50 mm, Angular blocky; Moderately moist; Weak consistence; Many cutans, >50%
	 of ped faces or walls coated; Gradual change to - 
	B21	0.96 - 1.04 m	Yellowish brown (10YR5/6-Moist); ; Medium heavy clay; Weak grade of structure, 100-200 mm, 
	Prismatic; 20-50 mm, Angular blocky; Moderately moist; Weak consistence; Very few (0 - 2 %), 
	Calcareous, , Tubules; Gradual change to - 
	B22	1.35 - 1.47 m	Yellowish brown (10YR5/6-Moist); , 7.5YR64; Medium clay; Strong grade of structure, Angular 
	blocky; Dry; Weak consistence; Many cutans, >50% of ped faces or walls coated; Very many (50
	 - 100 %), Ferromanganiferous, , ; Few (2 - 10 %), Calcareous, Very coarse (20 - 60 mm), 
	Tubules; Gradual change to - 

	Project Name:	WAG
	Project Code:	WAG	Site ID:	C39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	B23	1.7 - 1.83 m	Yellowish brown (10YR5/6-Moist); , 7.5YR64; Medium clay; Strong grade of structure, 20-50 mm,
	 Angular blocky; Strong grade of structure, 2-5 mm, Angular blocky; Dry; Weak consistence; 
	Many cutans, >50% of ped faces or walls coated; Very many (50 - 100 %), Ferromanganiferous, ,
	 ; Common (10 - 20 %), Calcareous, , Tubules; Sharp change to - 
	2A	2.21 - 2.31 m	Reddish yellow (7.5YR6/6-Moist); ; Light clay; 20-50 mm; Moderate grade of structure, 20-50 
	mm, Subangular blocky; Dry; Very firm consistence; Many cutans, >50% of ped faces or walls 
	coated; , Ferromanganiferous, , ; Very few (0 - 2 %), Calcareous, , Veins; Sharp change to - 
	2B	2.39 - 2.46 m	Yellowish brown (10YR5/4-Moist); ; Silty medium clay (Light); Strong grade of structure, Angular 
	blocky; Strong grade of structure, 5-10 mm, Angular blocky; Dry; Very weak consistence; Many 
	cutans, >50% of ped faces or walls coated; Very many (50 - 100 %), Ferromanganiferous, , ; Few
	 (2 - 10 %), Calcareous, , Tubules; Gradual change to - 
	3 - 3.15 m	Light brown (7.5YR6/4-Moist); ; , Angular blocky; Weak consistence; Gradual change to - 
	3.76 - 3.91 m	Light yellowish brown (10YR6/4-Moist); ; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; , 
	Ferruginous, , Concretions; 
	Morphological Notes
	Observation Notes
	Site Notes
	MITCHELL

	Project Name:	WAG
	Project Code:	WAG	Site ID:	C39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAG
	Project Code:	WAG	Site ID:	C39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile