Project Name:	WAG
	Project Code:	WAG	Site ID:	C40	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	E. Bettenay	Locality:	S.E. face of brick quarry Willie & Son Wagga Wagga:
	Date Desc.:	12/12/56	Elevation:	 189 metres
	Map Ref.:	Rainfall:	540
	Northing/Long.:	Runoff:	No Data
	Easting/Lat.:	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	6 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Hypercalcic Red Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.08 m	Brown (10YR4/3-Moist); , 7.5YR55; Silty clay loam; Weak grade of structure, 20-50 mm, Platy; 
	Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Weak consistence; 0-2%, fine 
	gravelly, 2-6mm, Quartz, coarse fragments; , fine (1-2mm) roots; 
	0.08 - 0.15 m	Reddish yellow (5YR6/6-Moist); , 2.5YR34; Silty clay loam; Weak grade of structure, 20-50 mm, 
	Angular blocky; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Very firm 
	consistence; 10-20%, Gravel, coarse fragments; 
	B	0.15 - 0.2 m	Red (2.5YR4/6-Moist); , 5YR66; Silty light clay; Weak grade of structure, 20-50 mm, Angular 
	blocky; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Very firm consistence; 0-
	2%, Gravel, coarse fragments; Very few (0 - 2 %), Ferruginous, , Nodules; 
	0.2 - 0.28 m	Red (2.5YR4/6-Moist); , 5YR56; Medium clay; Weak grade of structure, Angular blocky; Few (<1 
	per 100mm2) Very fine (0.075-1mm) macropores, Very firm consistence; 0-2%, Gravel, coarse 
	fragments; 
	0.28 - 0.36 m	Red (2.5YR4/6-Moist); ; Heavy clay; Weak grade of structure, 20-50 mm, Angular blocky; Weak 
	grade of structure, 10-20 mm, Angular blocky; Few (<1 per 100mm2) Very fine (0.075-1mm) 
	macropores, Very firm consistence; 0-2%, fine gravelly, 2-6mm, Gravel, coarse fragments; Few 
	(2 - 10 %), Argillaceous, Fine (0 - 2 mm), Nodules; 
	0.51 - 0.61 m	Red (2.5YR4/6-Moist); ; Heavy clay; Massive grade of structure; 20-50 mm, Angular blocky; Few 
	(<1 per 100mm2) Very fine (0.075-1mm) macropores, Very firm consistence; 2-10%, fine 
	gravelly, 2-6mm, Gravel, coarse fragments; , Argillaceous, Medium (2 -6 mm), Nodules; 
	BC	0.66 - 0.81 m	Reddish brown (5YR4/4-Moist); ; Medium heavy clay; Massive grade of structure; Dry; Very firm 
	consistence; 0-2%, fine gravelly, 2-6mm, Gravel, coarse fragments; Common cutans, 10-50% of 
	ped faces or walls coated; Very few (0 - 2 %), Argillaceous, Medium (2 -6 mm), Nodules; Few (2 
	- 10 %), Calcareous, , Soft segregations; 
	2B	0.91 - 1.02 m	Yellowish brown (10YR5/6-Moist); , 2.5YR46; Weak grade of structure, 20-50 mm, Angular 
	blocky; Dry; Weak consistence; Few (2 - 10 %), Calcareous, , Soft segregations; 
	1.68 - 1.83 m	Yellowish brown (10YR5/6-Moist); , 2.5YR46; 
	2.13 - 2.29 m	Red (2.5YR4/6-Moist); , 10YR56; , 5Y54; Very firm consistence; , Calcareous, , Veins; 

	Project Name:	WAG
	Project Code:	WAG	Site ID:	C40	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	3A	2.74 - 3.04 m	Greyish brown (10YR5/2-Moist); , 2.5YR46; Light clay; , Subangular blocky; Dry; Very firm 
	consistence; 
	3B	3.05 - 3.35 m	Brown (10YR4/3-Moist); , 2.5YR46; Heavy clay; 50-100 mm, Angular blocky; ; FragmentDry; Very 
	firm consistence; , Calcareous, , Veins; 
	3C	4.27 - 4.57 m	; Silty medium clay; Massive grade of structure; Dry; Very firm consistence; Few cutans, <10% 
	of ped faces or walls coated; 
	4A1	6.1 - 6.4 m	Bluish grey (5B5/1-Moist); , 5Y68; , Angular blocky; Few (<1 per 100mm2) Very fine (0.075-1mm) 
	macropores, Dry; Very firm consistence; 
	4A2	6.4 - 6.55 m	; 2-10%, coarse fragments; 
	4B	6.55 - 6.71 m	Yellowish brown (10YR5/6-Moist); , 10YR64; , 2.5YR46; , Angular blocky; Few (<1 per 100mm2) 
	Very fine (0.075-1mm) macropores, 2-10%, Gravel, coarse fragments; Common cutans, 10-50% 
	of ped faces or walls coated; 
	7.62 - 7.92 m	Yellowish brown (10YR5/6-Moist); ; 50-100 mm; Few (<1 per 100mm2) Very fine (0.075-1mm) 
	macropores, Weak consistence; 2-10%, Gravel, coarse fragments; 
	5A	0 - 0.3 m	Light yellowish brown (10YR6/4-Moist); ; Silty clay loam; 50-100 mm, Angular blocky; Common 
	(1-5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Very firm consistence; 
	5B1	0.3 - 0.46 m	Grey (10YR5/1-Moist); , 2.5YR46; Heavy clay; Massive grade of structure; Moderately moist; 
	Weak consistence; 
	5C	1.52 - 1.68 m	Grey (10YR6/1-Moist); , 10YR64; Light clay; Massive grade of structure; Common (1-5 per 
	100mm2) Very fine (0.075-1mm) macropores, Moderately moist; Weak consistence; 
	2.44 - 2.59 m	Red (2.5YR4/6-Moist); , 2.5YR50; Silty light clay; Massive grade of structure; Common (1-5 per 
	100mm2) Very fine (0.075-1mm) macropores, Weak consistence; 
	Morphological Notes
	Observation Notes
	SAMPLES 18-21 ARE COLLECTED FROM S.W. FACE OF QUARRY: 213-305CM AL GRAVEL IS ATTAPULGITE: 213-427CM 
	WIDELY SPACE Ca     COLUMNS:
	Site Notes
	WYNARD

	Project Name:	WAG
	Project Code:	WAG	Site ID:	C40	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAG
	Project Code:	WAG	Site ID:	C40	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile