Project Name:	YEN
	Project Code:	YEN	Site ID:	C25	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	D.C. van Dijk	Locality:	Between main canal and Griffith - Tharbogang 
	Railway .8km west of raodto Lake Wyangan + 20m 
	south of Railway:
	Date Desc.:	08/12/55	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	Runoff:	No Data
	Easting/Lat.:	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Calcic Red Dermosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red-brown earth
	No analytical data and little or no knowledge of this soil.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.08 m	Red (2.5YR4/5-Moist); ; Fine sandy clay loam (Light); Moderate grade of structure, 20-50 mm, 
	Platy; Dry; Very firm consistence; 0-2%, Sandstone, coarse fragments; 
	A	0.08 - 0.2 m	Red (2.5YR5/6-Moist); ; Light clay (Light); Weak grade of structure, 10-20 mm, Angular blocky; 
	Dry; Very firm consistence; 0-2%, Gravel, coarse fragments; Gradual change to - 
	A/B	0.2 - 0.33 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Weak grade of structure, 10-20 mm, Angular 
	blocky; Dry; Firm consistence; 10-20%, Gravel, coarse fragments; Gradual change to - 
	B	0.36 - 0.48 m	Red (10R4/6-Moist); ; Medium clay; Weak grade of structure, 20-50 mm, Prismatic; Moderate 
	grade of structure, 5-10 mm, Angular blocky; Dry; Firm consistence; Few (2 - 10 %), Unidentified,
	 Medium (2 -6 mm), ; Sharp change to - 
	0.53 - 0.79 m	Red (10R4/5-Moist); , 5YR56, 2-10% ; , 2-10% ; Coarse sandy medium clay; Massive grade of 
	structure; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Strong consistence; 
	Very plastic; Subplastic; 
	0.89 - 1.14 m	Dark yellowish brown (10YR4/5-Moist); , 10YR55; Moderate grade of structure, 50-100 mm, Platy;
	 Strong consistence; Very plastic; Subplastic; , Calcareous, , Soft segregations; Gradual 
	change to - 
	1.52 - 1.75 m	Red (2.5YR4/6-Moist); , 10YR64; Very plastic; Subplastic; Common (10 - 20 %), Calcareous, , 
	Concretions; 
	Morphological Notes
	Observation Notes
	0-8CM GRAVEL Fe INDURATED: 53-114CM AGGREGATES WITH WHITE COATING AND  SOME BLACK STAINING:              
	               
	Site Notes
	COOPER

	Project Name:	YEN
	Project Code:	YEN	Site ID:	C25	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	YEN
	Project Code:	YEN	Site ID:	C25	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile