Project Name:	CAN
	Project Code:	CAN	Site ID:	C142	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	H.M. Churchwood	Locality:	~20M west of C141
	Date Desc.:	01/12/56	Elevation:	 85 metres
	Map Ref.:	Sheet No. : 7627   1:100000	Rainfall:	325
	Northing/Long.:	143.583333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-35.2	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epihypersodic Petroclcic Leptic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Tall Strata - Malle shrub, , . *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	0 - 0.08 m	Strong brown (7.5YR5/6-Moist); ; Sandy clay loam (Light); 5-10 mm, Angular blocky; Weak grade 
	of structure, 10-20 mm, Angular blocky; Very weak consistence; Field pH 8.5 (pH meter); 
	0.08 - 0.18 m	Yellowish red (5YR5/6-Moist); ; Sandy clay loam; 5-10 mm, Angular blocky; Weak grade of 
	structure, 10-20 mm, Angular blocky; Very weak consistence; Few (2 - 10 %), Calcareous, , Soft 
	segregations; Field pH 9.4 (pH meter); 
	0.18 - 0.33 m	Yellowish red (5YR4/6-Moist); ; Sandy light clay; 5-10 mm, Angular blocky; Weak grade of 
	structure, 10-20 mm, Angular blocky; Firm consistence; Few (2 - 10 %), Calcareous, , Soft 
	segregations; Field pH 9.5 (pH meter); 
	B	0.41 - 0.51 m	Strong brown (7.5YR5/6-Moist); ; Sandy light clay (Heavy); Dry; Firm consistence; Very few (0 - 2 
	%), Calcareous, , Soft segregations; Calcrete, Weakly cemented; Field pH 9.5 (pH meter); 
	Bk	0.66 - 0.76 m	Yellowish red (5YR5/8-Moist); ; Sandy light clay (Heavy); Moderately moist; Weak consistence; 
	Very few (0 - 2 %), Calcareous, , Soft segregations; Calcrete, Very strongly cemented; Field pH 
	9.2 (pH meter); 
	Bk	0.97 - 1.07 m	Reddish yellow (5YR6/8-Moist); ; Sandy light clay (Heavy); Moderately moist; Weak consistence;
	 Calcrete, Very strongly cemented; Field pH 9.2 (pH meter); 
	Bk	1.42 - 1.52 m	Reddish yellow (5YR6/8-Moist); ; Light clay; Dry; Weak consistence; Calcrete, Very strongly 
	cemented; Field pH 9.2 (pH meter); 
	Bk	2.18 - 2.29 m	Yellowish red (5YR5/8-Moist); ; Light clay (Heavy); Dry; Firm consistence; Calcrete, Moderately 
	cemented; Field pH 9.3 (pH meter); 
	2.95 - 3.05 m	Yellowish red (5YR5/8-Moist); ; Medium clay; Weak consistence; Calcrete, Weakly cemented; 
	Field pH 9.1 (pH meter); 
	3.56 - 3.66 m	Reddish brown (5YR4/3-Moist); ; Medium clay (Heavy); Firm consistence; Field pH 8.6 (pH 
	meter); 
	Morphological Notes
	Observation Notes
	LAYERS RE NUMBERED 19/10/92                                                                                             

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C142	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Notes
	MURRAKOOL

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C142	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8.5A	 0.089A	 10.7K	 2.3	 1.9	 0.21	 15.1B
	0.08 - 0.18	9.4A	 0.179A	 10.9K	 3.6	 2	 1.5	 18B
	0.18 - 0.33	9.5A	 0.536A
	0.41 - 0.51	9.5A	 0.833A	 5.8K	 5.7	 1.5	 4.7	 17.7B
	0.66 - 0.76	9.2A	 1.9A
	0.97 - 1.07	9.2A	 2.26A	 2.6K	 6.7	 1.1	 3.9	 14.3B
	1.42 - 1.52	9.2A	 1.73A
	2.18 - 2.29	9.3A	 1.49A
	2.95 - 3.05	9.1A	 1.73A
	3.56 - 3.66	8.6A	 1.87A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.07A	 42D	 36	 8	 13
	0.08 - 0.18	 0.52A	 34D	 35	 11	 20
	0.18 - 0.33	 3.52A	 36D	 29	 10	 23
	0.41 - 0.51	 5.31A	 34D	 30	 10	 25
	0.66 - 0.76	 19.1A	 30D	 27	 12	 29
	0.97 - 1.07	 21A	 29D	 29	 11	 31
	1.42 - 1.52
	2.18 - 2.29	 34.2A	 27D	 29	 8	 37
	2.95 - 3.05
	3.56 - 3.66	 0.75A	 27D	 28	 8	 37
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.18
	0.18 - 0.33
	0.41 - 0.51
	0.66 - 0.76
	0.97 - 1.07
	1.42 - 1.52
	2.18 - 2.29
	2.95 - 3.05
	3.56 - 3.66

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C142	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance