Project Name:	CAN
	Project Code:	CAN	Site ID:	CP97	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	P.A. Boyd	Locality:
	Date Desc.:	05/10/77	Elevation:	 160 metres
	Map Ref.:	Sheet No. : 7425   1:100000	Rainfall:	420
	Northing/Long.:	141.566666666667	Runoff:	Slow
	Easting/Lat.:	-36.4333333333334	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Low hills
	10%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Mesonatric Red Sodosol     	Principal Profile Form:	Dr2.33
	ASC Confidence:	Great Soil Group:	Red-brown earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Brown (7.5YR5/4-Dry); ; Sandy loam; Field pH 6.2 (pH meter); 
	0.05 - 0.1 m	Brown (7.5YR5/4-Dry); ; Sandy loam; Field pH 6.5 (pH meter); 
	0.1 - 0.2 m	Reddish brown (5YR4/3-Dry); , 7.5YR64; Medium clay; Field pH 7.3 (pH meter); 
	0.2 - 0.3 m	Reddish brown (5YR4/3-Dry); ; Medium clay; Field pH 8.1 (pH meter); 
	0.3 - 0.4 m	Reddish brown (5YR4/3-Dry); ; Medium clay; Field pH 8.6 (pH meter); 
	0.4 - 0.5 m	Brown (7.5YR5/4-Dry); ; Light clay; Few (2 - 10 %), Calcareous, , Concretions; Field pH 8.7 (pH 
	meter); Gradual change to - 
	0.5 - 0.6 m	Brown (7.5YR5/4-Dry); ; Light clay; Few (2 - 10 %), Calcareous, , Concretions; Field pH 8.9 (pH 
	meter); 
	0.6 - 0.8 m	; Light clay; Few (2 - 10 %), Calcareous, , Concretions; Field pH 9 (pH meter); Gradual change to
	 - 
	0.8 - 1 m	, 10YR63; Light clay; Few (2 - 10 %), Calcareous, , Concretions; Field pH 9.2 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	NHILL

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP97	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.2A	 0.07A	 2.6K	 1.5	 1.3	 0.51	 10.7B	 16.7J	3.05
	0.05 - 0.1	6.5A	 0.05A
	0.1 - 0.2	7.3A	 0.02A	 4.3K	 4.2	 1.4	 4.2	 9.9B	 24J	17.50
	0.2 - 0.3	8.1A	 0.64A
	0.3 - 0.4	8.6A	 0.92A
	0.4 - 0.5	8.7A	 1.1A
	0.5 - 0.6	8.9A	 1.5A
	0.6 - 0.8	9A	 1.5A
	0.8 - 1	9.2A	 1.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.8
	0.8 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.8
	0.8 - 1

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP97	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour