Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A931	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	09/06/64	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	141.33333333	Runoff:	Rapid
	Easting/Lat.:	-36.38333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Rolling rises 9-30m 10-32%	Pattern Type:	Rises
	Morph. Type:	Ridge	Relief:	24 metres
	Elem. Type:	Scroll	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous-Epihypersodic Epipedal Black Vertosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Black earth
	No analytical data and little or no knowledge of this soil.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Tall Strata - , , . *Species includes - Eucalyptus species, Casuarina leuhmannii
	Surface Coarse Fragments:
	Profile Morphology
	0.3 - 0.38 m	; Medium clay; , Columnar; Coarse, (10 - 20) mm crack; Diffuse change to - 
	0.5 - 0.6 m	; Medium clay; Strong consistence; Diffuse change to - 
	0.65 - 0.73 m	; Medium clay; Strong consistence; Diffuse change to - 
	0.73 - 0.78 m	; Medium clay; Strong consistence; Diffuse change to - 
	0.78 - 0.93 m	; Medium clay; Strong consistence; Diffuse change to - 
	0.98 - 1.13 m	; Medium clay; Strong consistence; Diffuse change to - 
	1.2 - 1.35 m	; Medium clay; Strong consistence; Field pH 8 (pH meter); Diffuse change to - 
	1.43 - 1.55 m	; Sandy medium clay; 0-2%, Gravel, coarse fragments; Field pH 8 (pH meter); Diffuse change to 
	- 
	1.65 - 1.88 m	; Medium clay; 0-2%, Gravel, coarse fragments; Field pH 7 (pH meter); Diffuse change to - 
	1.96 - 2.08 m	; Medium clay; 0-2%, Gravel, coarse fragments; Diffuse change to - 
	2.08 - 2.23 m	; Medium clay; Field pH 6 (pH meter); Diffuse change to - 
	2.23 - 2.38 m	; Sandy medium clay; Field pH 6 (pH meter); 
	2.38 - 2.63 m	; Sandy medium clay; 
	2.63 - 2.83 m	; Sandy clay loam; Field pH 5 (pH meter); 
	2.83 - 2.88 m	; 
	2.8 - 3.1 m	; Rigid consistence; 
	3.4 - 3.7 m	; Very strong consistence; 
	4 - 4.3 m	; Very strong consistence; 

	Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A931	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	4.6 - 4.9 m	; 
	Morphological Notes
	280 cm+ sandstone:
	Observation Notes
	208-238CM CLAY SKINS:                                                                                                   
	Site Notes
	LOWAN

	Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A931	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.3 - 0.38	9.3H	 0.084C
	0.5 - 0.6	9.6H	 0.18C
	0.65 - 0.73	9.8H	 0.22C
	0.73 - 0.78	9.6H	 0.29C
	0.78 - 0.93	9.5H	 0.35C
	0.98 - 1.13	9.4H	 0.39C
	1.2 - 1.35	9.3H	 0.8C
	1.43 - 1.55	9.1H	 0.41C
	1.65 - 1.88	8.7H	 0.56C
	1.96 - 2.08	8.3H	 0.65C
	2.08 - 2.23	7.4H	 0.53C
	2.23 - 2.38	6.4H	 0.35C
	2.38 - 2.63	6.7H	 0.31C
	2.63 - 2.83	6.5H	 0.28C
	2.83 - 2.88	6.6H	 0.27C
	2.8 - 3.1
	3.4 - 3.7
	4 - 4.3
	4.6 - 4.9	5.1H	 0.14C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.3 - 0.38	 20C	 7	 10C	 21	 6	 42
	0.5 - 0.6	 22C
	0.65 - 0.73	 17C
	0.73 - 0.78	 14C	 16	 17C	 26	 6	 37
	0.78 - 0.93	 8.7C
	0.98 - 1.13	 5C
	1.2 - 1.35	 1.3C	 1	 22C	 35	 7	 35
	1.43 - 1.55	 0.17C
	1.65 - 1.88	 0.1C	 23C	 31	 7	 38
	1.96 - 2.08	 0.14C
	2.08 - 2.23	 0.01C	 25C	 32	 4	 40
	2.23 - 2.38	 0.01C
	2.38 - 2.63	 0.01C
	2.63 - 2.83	 0.01C	 40C	 34	 2	 24
	2.83 - 2.88	 0.01C
	2.8 - 3.1
	3.4 - 3.7
	4 - 4.3
	4.6 - 4.9	 0.01C	 57C	 31	 2	 10
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.3 - 0.38
	0.5 - 0.6
	0.65 - 0.73

	Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A931	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	0.73 - 0.78
	0.78 - 0.93
	0.98 - 1.13
	1.2 - 1.35
	1.43 - 1.55
	1.65 - 1.88
	1.96 - 2.08
	2.08 - 2.23
	2.23 - 2.38
	2.38 - 2.63
	2.63 - 2.83
	2.83 - 2.88
	2.8 - 3.1
	3.4 - 3.7
	4 - 4.3
	4.6 - 4.9

	Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A931	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_St	Smectite - X-Ray Diffraction