Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A934	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	11/06/64	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	141.51666667	Runoff:	Rapid
	Easting/Lat.:	-36.4	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Ridge	Relief:	9 metres
	Elem. Type:	Embankment	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Class Undetermined Regolithic Calcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Brown clay
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Highly disturbed, for example, quarrying, roadworks, mining, landfill, urban
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	; Medium clay; , Columnar; Very firm consistence; Common (10 - 20 %), Calcareous, , Soft 
	segregations; 
	0.15 - 0.3 m	; Medium clay; , Columnar; Strong consistence; Common (10 - 20 %), Calcareous, , Soft 
	segregations; Diffuse change to - 
	0.3 - 0.48 m	; Medium clay; , Columnar; Very strong consistence; Common (10 - 20 %), Calcareous, , Soft 
	segregations; Diffuse change to - 
	0.48 - 0.63 m	; Medium clay; , Columnar; Very strong consistence; Very few (0 - 2 %), Calcareous, , Soft 
	segregations; 
	0.63 - 0.8 m	; Sandy medium clay; , Columnar; Very strong consistence; Common (10 - 20 %), Calcareous, , 
	Soft segregations; 
	0.8 - 1.05 m	; Sandy medium clay; , Columnar; Very strong consistence; 0-2%, Gravel, coarse fragments; 
	Very few (0 - 2 %), Calcareous, , Soft segregations; Field pH 9 (pH meter); 
	1.05 - 1.3 m	; Sandy medium clay; , Columnar; Very strong consistence; 0-2%, Gravel, coarse fragments; 
	Very few (0 - 2 %), Calcareous, , Soft segregations; Field pH 9 (pH meter); 
	1.3 - 1.68 m	; Sandy clay loam; Field pH 8 (pH meter); 
	1.8 - 1.88 m	; Sandy medium clay; , Columnar; Very strong consistence; Field pH 6 (pH meter); 
	1.88 - 2.11 m	; Sandy medium clay; Very strong consistence; Field pH 6 (pH meter); 
	2.29 - 2.47 m	; Medium clay; Very strong consistence; Field pH 6 (pH meter); 
	2.47 - 2.82 m	; Very strong consistence; 
	2.89 - 3.19 m	; 
	4.27 - 4.57 m	; 
	Morphological Notes
	sandstone on face of quarry:

	Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A934	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	15-63CM CLAY SKINS: MUCH CALCIUM FROM 68-76CM:                                                                          
	Site Notes
	LOWAN
	Observation Notes

	Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A934	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.4H	 0.049C
	0.15 - 0.3	8.7H	 0.059C
	0.3 - 0.48	9.2H	 0.073C
	0.48 - 0.63	9.3H	 0.11C
	0.63 - 0.8	9.1H	 0.22C
	0.8 - 1.05	9.1H	 0.29C
	1.09 - 1.35	9.1H	 0.28C
	1.35 - 1.7	8.9H	 0.22C
	1.82 - 2.01	8.5H	 0.3C
	2.01 - 2.24	7.8H	 0.24C
	2.29 - 2.47	6.8H	 0.27C
	2.47 - 2.82	6.7H	 0.19C
	2.89 - 3.19	7.6H	 0.071C
	4.27 - 4.57
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 7.4C	 25C	 23	 5	 38
	0.15 - 0.3	 10C
	0.3 - 0.48	 9.3C	 24C	 21	 5	 40
	0.48 - 0.63	 0.93C
	0.63 - 0.8	 7.4C	 22C	 22	 5	 43
	0.8 - 1.05	 3.9C
	1.09 - 1.35	 0.49C	 32C	 25	 6	 37
	1.35 - 1.7	 0.03C
	1.82 - 2.01	 0.05C	 32C	 24	 7	 37
	2.01 - 2.24	 0.01C	 39C	 24	 4	 32
	2.29 - 2.47	 0.01C	 36C	 19	 7	 38
	2.47 - 2.82	 0.01C	 48C	 18	 8	 20
	2.89 - 3.19	 0.01C	 60C	 17	 4	 7
	4.27 - 4.57
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.15 - 0.3
	0.3 - 0.48
	0.48 - 0.63
	0.63 - 0.8
	0.8 - 1.05
	1.09 - 1.35
	1.35 - 1.7
	1.82 - 2.01
	2.01 - 2.24
	2.29 - 2.47
	2.47 - 2.82
	2.89 - 3.19

	Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A934	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	4.27 - 4.57

	Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A934	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_St	Smectite - X-Ray Diffraction