Project Name:	LSG
	Project Code:	LSG	Site ID:	CP62	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	J.R. Sleeman	Locality:	Padock 9 to 10M S.W. of pump. site:
	Date Desc.:	22/06/76	Elevation:	 80 metres
	Map Ref.:	Sheet No. : 7626   1:100000	Rainfall:	360
	Northing/Long.:	143.966666666667	Runoff:	Slow
	Easting/Lat.:	-35.7666666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Level
	Slope:	0 % 	Aspect:	200 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epihypersodic-Endoacidic Massive Brown Vertosol     	Principal Profile Form:	Ug5.5
	ASC Confidence:	Great Soil Group:	Brown clay
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Light medium clay; Massive grade of structure; Very 
	strong consistence; Field pH 7.3 (pH meter); Common
	0.1 - 0.2 m	Brown (10YR4/3-Moist); ; Light medium clay; , Angular blocky; Very firm consistence; Field pH 
	8.1 (pH meter); 
	0.2 - 0.3 m	Brown (10YR5/3-Moist); ; Light medium clay; Massive grade of structure; Weak consistence; 
	Field pH 8 (pH meter); 
	0.3 - 0.4 m	Yellowish brown (10YR5/4-Moist); ; Light medium clay; Massive grade of structure; Very weak 
	consistence; Field pH 8.2 (pH meter); 
	0.4 - 0.5 m	Yellowish brown (10YR5/4-Moist); ; Light medium clay; Massive grade of structure; Very weak 
	consistence; 
	0.5 - 0.6 m	Light yellowish brown (10YR6/4-Moist); ; Light medium clay; Massive grade of structure; Very 
	weak consistence; Field pH 8.3 (pH meter); 
	0.6 - 0.7 m	Light yellowish brown (10YR6/4-Moist); ; Light medium clay; Massive grade of structure; Weak 
	consistence; , Gypseous, Medium (2 -6 mm), Soft segregations; 
	0.7 - 0.8 m	Light yellowish brown (10YR6/4-Moist); ; Light medium clay; Massive grade of structure; Weak 
	consistence; , Gypseous, Medium (2 -6 mm), Soft segregations; Field pH 7.5 (pH meter); 
	0.8 - 0.9 m	Light yellowish brown (10YR6/4-Moist); ; Light medium clay; Massive grade of structure; Weak 
	consistence; , Gypseous, Medium (2 -6 mm), Soft segregations; 
	0.9 - 1 m	Light yellowish brown (10YR6/4-Moist); ; Light medium clay; Massive grade of structure; Weak 
	consistence; , Gypseous, Medium (2 -6 mm), Soft segregations; Field pH 7.9 (pH meter); 
	1 - 1.1 m	Light yellowish brown (10YR6/4-Moist); , 2.5YR54, 2-10% ; , 2-10% ; Light medium clay; Massive
	 grade of structure; Weak consistence; , Gypseous, Medium (2 -6 mm), Soft segregations; 
	1.1 - 1.2 m	Light yellowish brown (10YR6/4-Moist); , 2.5YR54, 10-20% ; , 10-20% ; Light medium clay; 
	Massive grade of structure; Weak consistence; , Gypseous, Medium (2 -6 mm), Soft 
	segregations; 

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP62	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	1.2 - 1.3 m	Light yellowish brown (10YR6/4-Moist); , 2.5YR54, 10-20% ; , 10-20% ; Light medium clay; 
	Massive grade of structure; Weak consistence; , Gypseous, Medium (2 -6 mm), Soft 
	segregations; 
	Morphological Notes
	Observation Notes
	GLOSSY SURFACES 30-90CM:"PIPES"(30-90CM) MN STAINING ON SHINY FACES:HORIZONTAL BAND AT 2-4CM:                
	           
	Site Notes
	KERANG FARM

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP62	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.3A	 0.26A	 9K	 7.6	 1	 3.6	 8.1B	 29.3J	12.29
	0.1 - 0.2	8.1A	 0.6A	 12.4K	 12	 0.92	 7	 6.4B	 38.7J	18.09
	0.2 - 0.3	8A	 0.92A	 11K	 12.6	 1.2	 7.5	 5.1B	 37.4J	20.05
	0.3 - 0.4	8.2A	 1.1A	 9K	 12.6	 1	 8.2	 4.7B	 35.5J	23.10
	0.5 - 0.6	8.3A	 1.4A	 8.5K	 11.4	 1	 8.7	 3.2B	 32.7J	26.61
	0.7 - 0.8	7.5A	 3.6A	 8.8K	 10.1	 1	 9	 1.1B	 30J	30.00
	0.9 - 1	7.9A	 3.1A	 8.1K	 10.3	 1	 8.4	 2.5B	 30.3J	27.72
	1.1 - 1.2	8A	 3.2A	 7.6K	 9.8	 0.93	 9.6	 1.9B	 29.8J	32.21
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.9D	 0D	 28	 21	 50
	0.1 - 0.2	 0.08A	 0.72D	 0D	 15	 24	 64
	0.2 - 0.3	 0.09A	 0.63D	 0D	 13	 24	 64
	0.3 - 0.4	 0.1A	 0.41D	 0D	 15	 16	 70
	0.5 - 0.6	 0.47A	 0.17D	 0D	 14	 18	 67
	0.7 - 0.8	 0.11D	 0D	 14	 20	 63
	0.9 - 1	 0.13A	 0.1D	 0D	 14	 21	 63
	1.1 - 1.2	 3A	 0.08D	 0D	 12	 23	 63
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.5 - 0.6
	0.7 - 0.8
	0.9 - 1
	1.1 - 1.2

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP62	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance