Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	G. Blackburn	Locality:	IMPROVED SUB-CLOVER PASTURE
	Date Desc.:	17/11/53	Elevation:	 170 metres
	Map Ref.:	1:250000	Rainfall:	610
	Northing/Long.:	141.366666666667	Runoff:	Very slow
	Easting/Lat.:	-37.2	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Plateau
	1-3%
	Morph. Type:	No Data	Relief:	15 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Grey Sodosol     	Principal Profile Form:	Dy3.83
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, 20.01-35m, Very sparse. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Greyish brown (10YR5/2-Moist); , 10YR56; Sandy loam; Weak consistence; Few (2 - 10 %), 
	Ferruginous, , Concretions; Diffuse change to - 
	0.08 - 0.15 m	Light brownish grey (10YR6/2-Moist); , 10YR56; Sandy loam; Weak consistence; Few (2 - 10 %),
	 Ferruginous, , Concretions; Diffuse change to - 
	0.15 - 0.23 m	Grey (10YR6/1-Moist); , 10YR56; Loamy sand; Massive grade of structure; Very firm 
	consistence; Very few (0 - 2 %), Ferruginous, , Concretions; Diffuse change to - 
	0.23 - 0.3 m	Grey (10YR6/1-Moist); , 10YR56; Sand; Few (2 - 10 %), Ferruginous, , Concretions; Clear, Wavy 
	change to - 
	0.3 - 0.38 m	Grey (10YR6/1-Moist); , 10YR56; Medium clay; Massive grade of structure; Few (2 - 10 %), 
	Ferruginous, , Concretions; Diffuse change to - 
	0.38 - 0.59 m	Grey (10YR6/1-Moist); , 10YR56; Medium clay; Massive grade of structure; Very few (0 - 2 %), 
	Ferruginous, , Concretions; Diffuse change to - 
	0.59 - 0.91 m	Grey (10YR6/1-Moist); , 10YR56; Medium clay; Massive grade of structure; Very few (0 - 2 %), 
	Ferruginous, , Concretions; Diffuse change to - 
	0.91 - 1.24 m	Grey (10YR6/1-Moist); , 10YR56; Medium clay; Very firm consistence; Very few (0 - 2 %), 
	Ferruginous, , Concretions; Diffuse change to - 
	1.24 - 1.52 m	Brownish yellow (10YR6/6-Moist); ; Medium clay; Very firm consistence; 0-2%, medium gravelly, 
	6-20mm, Quartz, coarse fragments; Very few (0 - 2 %), Ferruginous, , Concretions; Few (2 - 10 
	%), Gypseous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	Site Notes
	LOWAN S & L.U. No 17. Map Site 1

	Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.8A	 0.015C
	0.08 - 0.15	5.9A	 0.011C
	0.15 - 0.23	6.3A	 0.008C
	0.23 - 0.3	6.6A	 0.007C
	0.3 - 0.38	6.7A	 0.013C
	0.38 - 0.59	6.4A	 0.026C
	0.59 - 0.91	6.2A	 0.168C
	0.91 - 1.24	7.9A	 0.179C
	1.24 - 1.52	8.4A	 0.288C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.15	 13	 16C	 56	 17	 9
	0.15 - 0.23
	0.23 - 0.3
	0.3 - 0.38
	0.38 - 0.59
	0.59 - 0.91
	0.91 - 1.24
	1.24 - 1.52
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.15 - 0.23
	0.23 - 0.3
	0.3 - 0.38
	0.38 - 0.59
	0.59 - 0.91
	0.91 - 1.24
	1.24 - 1.52

	Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A1	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded