Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A19	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	24/11/53	Elevation:	 152 metres
	Map Ref.:	1:250000	Rainfall:	530
	Northing/Long.:	141.504166666667	Runoff:	Rapid
	Easting/Lat.:	-36.8188888888889	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Ridge	Relief:	18 metres
	Elem. Type:	Lunette	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Hypercalcic Brown Chromosol     	Principal Profile Form:	Dr2.33
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Yellowish brown (10YR5/4-Moist); ; Sandy loam; , Granular; Very weak consistence; Many, fine 
	(1-2mm) roots; 
	0.08 - 0.15 m	Dark brown (10YR3/3-Moist); , 10YR44; Medium clay; Very weak consistence; 
	0.45 - 0.5 m	Very pale brown (10YR8/4-Moist); ; Very weak consistence; Many (20 - 50 %), Calcareous, , Soft 
	segregations; 
	0.95 - 1 m	; Many (20 - 50 %), Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	Site Notes
	LOWAN S & L.U. No 17. Map Site 19

	Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A19	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.7A	 0.011C	 5.3F	 1.1	 0.76	 0.12
	0.08 - 0.15	7.2A	 0.017C	 16.9F	 5.3	 2	 0.22	 5.4C
	0.45 - 0.5	8.7A	 0.057C
	0.95 - 1	9.3A	 0.066C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.008F	 0.09C	 42C	 38	 7	 12
	0.08 - 0.15	 0.011F	 0.123C	 28C	 20	 3	 50
	0.45 - 0.5	 39A	 11C	 7	 2	 39
	0.95 - 1	 26A	 19C	 12	 2	 41
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.45 - 0.5
	0.95 - 1

	Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A19	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. acidity By titration to pH 8.4
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7_C_B	Total Nitrogen - method description not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction