Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	21/11/53	Elevation:	 150 metres
	Map Ref.:	1:250000	Rainfall:	550
	Northing/Long.:	141.149166666667	Runoff:	Very slow
	Easting/Lat.:	-36.8052777777778	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Flat	Relief:	3 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Mottled-Hypernatric Brown Sodosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:	Low Strata - Sedge, , . *Species includes - None recorded
	Mid Strata - Shrub, , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus baxteri, Eucalyptus viminalis
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Grey (10YR6/1-Moist); ; Sand; Single grain grade of structure; Common, very fine (0-1mm) roots; 
	Diffuse change to - 
	0.08 - 0.15 m	Light grey (10YR7/1-Moist); ; Sand; Loose consistence; Many, coarse (>5mm) roots; 
	0.15 - 0.28 m	Light grey (10YR7/1-Moist); ; Sand; Loose consistence; Many, coarse (>5mm) roots; 
	0.28 - 0.5 m	Light grey (10YR7/1-Moist); , 10YR31; Sand; Loose consistence; Common, fine (1-2mm) roots; 
	Diffuse, Irregular change to - 
	0.5 - 0.65 m	Very pale brown (10YR7/4-Moist); , 10YR64; , 10YR32; Sand; Loose consistence; 2-10%, Sand,
	 coarse fragments; Abrupt change to - 
	0.65 - 0.73 m	Yellowish brown (10YR5/6-Moist); , 10YR51; Sandy clay loam; , Columnar; Massive grade of 
	structure; 2-10%, Sand, coarse fragments; Diffuse change to - 
	0.73 - 0.9 m	Yellowish brown (10YR5/4-Moist); , 10R56; , 10YR51; Sandy medium clay; Massive grade of 
	structure; Strong consistence; Calcrete; 
	0.9 - 1.18 m	Yellow (10YR7/6-Moist); , 5Y63; Sandy medium clay; Massive grade of structure; Very firm 
	consistence; 
	1.18 - 1.43 m	Yellow (10YR7/6-Moist); , 5Y63; Sandy medium clay; Massive grade of structure; Very firm 
	consistence; 2-10%, Limestone, coarse fragments; Common (10 - 20 %), Calcareous, , Soft 
	segregations; 
	Morphological Notes
	Observation Notes
	TOP OF CLAY UNEVEN THROUGH 2.5CM WITH CRACKS WITH GREY MATERIAL & BLEACHED CAPPINGS 1CM THICK    
	                       
	Site Notes
	LOWAN S & L.U. No 17. Map Site 5

	Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)

	Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.1A	 0.003C	 0.5F	 0.2	 0.01	 0.03
	0.08 - 0.15	5.6A	 0.003C
	0.15 - 0.28	5.7A	 0.005C
	0.28 - 0.5	6A	 0.005C
	0.5 - 0.65	6.7A	 0.01C
	0.65 - 0.73	7.3A	 0.036C	 1.7F	 3.5	 0.11	 2.2
	0.73 - 0.9	8.2A	 0.084C
	0.9 - 1.18	8.6A	 0.102C
	1.18 - 1.43	9.7A	 0.179C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.001F	 0.018C
	0.08 - 0.15	 42C	 57	 0	 1
	0.15 - 0.28
	0.28 - 0.5
	0.5 - 0.65	 0.002F	 0.019C
	0.65 - 0.73	 0.003F	 0.036C
	0.73 - 0.9
	0.9 - 1.18
	1.18 - 1.43
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.15 - 0.28
	0.28 - 0.5
	0.5 - 0.65
	0.65 - 0.73
	0.73 - 0.9
	0.9 - 1.18
	1.18 - 1.43

	Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7_C_B	Total Nitrogen - method description not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded