Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	103	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	10/08/90	Elevation:	200 metres
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7669224 AMG zone: 55	Runoff:	Very rapid
	Easting/Lat.:	481386  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, Sandstone 
	Land Form
	Rel/Slope Class: 	Steep low hills 30-90m 32-56%	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Steep
	Slope:	33 % 	Aspect:	340 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Brown Kandosol Medium Very gravelly 	Principal Profile Form:	Gn2.44
	Loamy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Yellow earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Acacia species, Erythroxylon australe
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Acacia shirleyi, Acacia species
	Surface Coarse Fragments:	90-100%, cobbly, 60-200mm, angular, 
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Sandy loam (Heavy); Massive grade of structure; Earthy 
	fabric; Dry; Weak consistence; 90-100%, coarse gravelly, 20-60mm, rounded, dispersed, 
	Sandstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Common, fine (1-2mm) roots; 
	Gradual, Smooth change to - 
	A2	0.1 - 0.28 m	Brown (10YR4/3-Moist); ; Sandy loam (Heavy); Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; 90-100%, coarse gravelly, 20-60mm, rounded, dispersed, Sandstone, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Few, fine (1-2mm) roots; Clear, Smooth 
	B21	0.28 - 0.7 m	Strong brown (7.5YR4/6-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; 90-100%, coarse gravelly, 20-60mm, rounded, dispersed, 
	Sandstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 4.5 (Raupach, 0.4); 
	Clear, Tongued change to - 
	C	0.7 - 0.8 m	; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	103	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.5A	0.89B	0.28	0.36	0.04
	0.28 - 0.7	5A	0.7B	0.53	0.23	0.09	2.8I	3.21
	1.8J	0.6	0.9	0.1	3.57
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.28 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.28 - 0.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	103	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension