Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	110	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	21/08/90	Elevation:	740 metres
	Map Ref.:	Sheet No. : 8159   GPS	Rainfall:	No Data
	Northing/Long.:	7886942 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	406059  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Rolling low hills 30-90m 10-	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	200 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Dystrophic Yellow Chromosol Medium Non-gravelly 	Principal Profile Form:	Dy2.41
	Sandy Clayey Deep
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax, Eragrostis species, Themeda 
	triandra	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Acacia species
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus citriodora, Eucalyptus acmenoides, Eucalyptus
	 terminalis
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.03 m	Dark greyish brown (10YR4/2-Moist); ; Loamy coarse sand; Single grain grade of structure; 
	Earthy fabric; Dry; Firm consistence; 0-2%, medium gravelly, 6-20mm, angular tabular, 
	dispersed, Rhyolite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Many, fine (1-2mm) roots;
	 Abrupt, Smooth change to - 
	A2c	0.03 - 0.18 m	Greyish brown (10YR5/2-Moist); ; Loamy coarse sand; Single grain grade of structure; Earthy 
	fabric; Dry; Firm consistence; 0-2%, medium gravelly, 6-20mm, angular tabular, dispersed, 
	Rhyolite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.05); 
	Common, very fine (0-1mm) roots; Abrupt, Smooth change to - 
	B1	0.18 - 0.25 m	Dark greyish brown (10YR4/2-Moist); ; Sandy clay loam (Heavy); Weak grade of structure, 20-50 
	mm, Angular blocky; Smooth-ped fabric; Moderately moist; Firm consistence; , Calcareous, , ; , 
	Gypseous, , ; Few, very fine (0-1mm) roots; Abrupt, Smooth change to - 
	B2	0.25 - 0.45 m	Brownish yellow (10YR6/6-Moist); Mottles, 5YR48, 10-20% , 5-15mm, Prominent; Mottles, 10-
	20% ; Light medium clay; Moderate grade of structure, 50-100 mm, Prismatic; Smooth-ped 
	fabric; Moderately moist; Firm consistence; Few cutans, <10% of ped faces or walls coated, 
	distinct; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.3); Gradual, Smooth change 
	to - 
	B3	0.45 - 1.2 m	Light brownish grey (2.5Y6/2-Moist); Substrate influence, 10R48, 20-50% , 15-30mm, Prominent;
	 Substrate influence, 5YR68, 20-50% ; Medium clay; Moderate grade of structure, 50-100 mm, 
	Prismatic; Smooth-ped fabric; Moderately moist; Firm consistence; , Calcareous, , ; , Gypseous,
	 , ; Field pH 5.5 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	110	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.03 - 0.18	5.2A	0.52B	0.64	0.26	0.06
	0.25 - 0.45	5.4A	0.4J	0.8	0.2	0.2	5.1I	3.92
	0.45 - 1.2	5.3A	0.36B	1	0.18	0.11
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.03 - 0.18
	0.25 - 0.45
	0.45 - 1.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.03 - 0.18
	0.25 - 0.45
	0.45 - 1.2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	110	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension