Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1112	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	19/05/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7811268 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	378753  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol Thick Gravelly Clayey Clayey 	Principal Profile Form:	Uf6.31
	Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Bothriochloa ewartiana, Bothriochloa decipiens, 
	Echinochloa species	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus erythrophloia, Eucalyptus papuana
	Surface Coarse Fragments:	10-20%, stony, 200-600mm, subrounded, Basalt
	Profile Morphology
	A11	0 - 0.12 m	Dark brown (7.5YR3/2-Moist); ; Light clay (Heavy); Weak grade of structure, 5-10 mm, Polyhedral;
	 Smooth-ped fabric; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.03); Gradual change to - 
	A12	0.12 - 0.45 m	Brown (7.5YR4/4-Moist); Mottles, 5YR44, 10-20% , Faint; Mottles, 10-20% ; Light clay; Weak 
	grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Few (2 - 10 %), Manganiferous, 
	Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Clear 
	change to - 
	B21	0.45 - 0.7 m	Reddish brown (5YR4/4-Moist); Mottles, 10YR44, 10-20% , 5-15mm, Faint; Mottles, 10-20% ; 
	Light clay (Heavy); Moderate grade of structure, 10-20 mm, Polyhedral; Smooth-ped fabric; Few 
	(2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 
	6.5 (Raupach, 0.55); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1112	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	7.5A
	0.12 - 0.45	7.2A
	0.45 - 0.7	7.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.12 - 0.45
	0.45 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.45
	0.45 - 0.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1112	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension