Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1113	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	19/05/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7807952 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	369988  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol Thick Non-gravelly Clayey 	Principal Profile Form:	Uf6.71
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa pertusa, Bothriochloa ewartiana, 
	Aristida species	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Isolated plants. *Species includes - Eucalyptus crebra, Eucalyptus papuana, Eucalyptus 
	melanophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.12 m	Dark reddish brown (5YR3/2-Moist); ; Light clay; Massive grade of structure; Earthy fabric; 2-10%,
	 medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; Few (2 - 10 %), 
	Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.05); Clear change to - 
	A12	0.12 - 0.3 m	Dark reddish brown (2.5YR3/4-Moist); ; Sandy light clay; Massive grade of structure; Earthy 
	fabric; 2-10%, medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; Few (2 - 10 %), 
	Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.25); Clear change to - 
	B21	0.3 - 0.6 m	Dark red (2.5YR3/6-Moist); ; Sandy light clay; Massive grade of structure; Earthy fabric; 2-10%, 
	medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; Few (2 - 10 %), 
	Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1113	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	7.1A	8.1B	3.1	0.93	0.08
	0.12 - 0.3	7.1A
	0.3 - 0.6	7.1A	5.4B	2.1	0.29	0.07
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.12 - 0.3
	0.3 - 0.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.3
	0.3 - 0.6

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1113	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension