Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1120	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	20/05/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7829017 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	343960  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Basalt 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endocalcareous Self-Mulching Black Vertosol Non-gravelly 	Principal Profile Form:	Ug5.12
	Medium fine Very fine Moderately deep 
	ASC Confidence:	Great Soil Group:	Black earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 1.01-3m, Sparse. *Species includes - Bothriochloa decipiens, Ophiurous exaltatus
	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra
	Surface Coarse Fragments:	0-2%, coarse gravelly, 20-60mm, subrounded, Basalt
	Profile Morphology
	A1	0 - 0.09 m	Dark reddish brown (5YR3/2-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, 
	Granular; Moist; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); Clear change to - 
	B21	0.09 - 0.45 m	Dark reddish brown (5YR3/2-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm,
	 Angular blocky; Moderately moist; Few cutans, <10% of ped faces or walls coated, distinct; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.4); Clear change to - 
	B3	0.45 - 0.8 m	Dark brown (7.5YR3/2-Moist); ; Light medium clay (Heavy); Moderate grade of structure, 10-20 
	mm, Subangular blocky; Dry; 2-10%, coarse gravelly, 20-60mm, subrounded, Basalt, coarse 
	fragments; Many (20 - 50 %), Calcareous, Coarse (6 - 20 mm), Nodules; , Gypseous, , ; Field pH 
	8.5 (Raupach, 0.7); Clear change to - 
	C	0.8 - 0.9 m	; Massive grade of structure; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1120	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.09	7.1A
	0.09 - 0.45	7.3A
	0.45 - 0.8	8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.09
	0.09 - 0.45
	0.45 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.09
	0.09 - 0.45
	0.45 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1120	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension