Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1123	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	21/05/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7802802 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	380467  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Terrace plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hemic Regolithic Orthic Tenosol Clay-loamy Sandy Very 	Principal Profile Form:	N/A
	deep  
	ASC Confidence:	Great Soil Group:	Alluvial soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Bothriochloa decipiens, Chloris gayana, 
	Heteropogon contortus	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus tessellaris, Eucalyptus tereticornis
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus tereticornis, Eucalyptus tessellaris
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Very dark grey (10YR3/1-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy fabric;
	 , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); Clear change to - 
	A12	0.1 - 0.35 m	Dark grey (10YR4/1-Moist); ; Loamy coarse sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.2); Clear change to - 
	2A1b	0.35 - 0.7 m	Very dark grey (10YR3/1-Moist); ; Silty clay loam; Massive grade of structure; Earthy fabric; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.5); Clear change to - 
	2A12	0.7 - 0.9 m	Dark brown (10YR3/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.8); Clear change to - 
	2A13	0.9 - 1.05 m	Yellowish brown (10YR5/4-Moist); ; Coarse sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 1); Clear change to - 
	1.05 - 1.5 m	Dark brown (10YR3/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 1.3); Clear change to - 
	1.5 - 2 m	Yellowish brown (10YR5/4-Moist); ; Coarse sand (Heavy); Single grain grade of structure; Sandy 
	(grains prominent) fabric; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 1.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1123	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	1.5 - 2	8.2A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	1.5 - 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	1.5 - 2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1123	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension