Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1124	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	21/05/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7802770 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	380759  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Gently inclined
	Slope:	7 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Supracalcic Subnatric Brown Sodosol Medium Non-gravelly 	Principal Profile Form:	Dy3.23
	Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Eragrostis species, Aristida species
	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eremophila mitchellii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus papuana, Acacia salicina, Eucalyptus crebra
	Surface Coarse Fragments:	50-90%, fine gravelly, 2-6mm, subangular, Quartz
	Profile Morphology
	A1	0 - 0.13 m	Light grey (10YR7/2-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Dry; 10-20%, medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.1); Clear change to - 
	A2	0.13 - 0.28 m	Brown (7.5YR5/4-Moist); ; Clayey sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Moderately moist; 10-20%, medium gravelly, 6-20mm, subrounded, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Abrupt change to - 
	B21	0.28 - 0.4 m	Light olive brown (2.5Y5/4-Moist); Mottles, 5YR46, 10-20% , 5-15mm, Prominent; Mottles, 10-
	20% ; Medium clay; Weak grade of structure; Smooth-ped fabric; Moist; , Calcareous, , ; , 
	Gypseous, , ; Field pH 8.5 (Raupach, 0.4); Gradual change to - 
	B22k	0.4 - 0.65 m	Light olive brown (2.5Y5/4-Moist); ; Medium clay; Weak grade of structure; Smooth-ped fabric; 
	Moderately moist; Common (10 - 20 %), Calcareous, Coarse (6 - 20 mm), Soft segregations; , 
	Gypseous, , ; Clear change to - 
	B23	0.65 - 0.75 m	; Sandy medium clay; Weak grade of structure; Smooth-ped fabric; 2-10%, medium gravelly, 6-
	20mm, subrounded, Quartz, coarse fragments; Common (10 - 20 %), Calcareous, Coarse (6 - 20 
	mm), Soft segregations; , Gypseous, , ; Field pH 9.5 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1124	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	6.6A	1.6B	1	0.29	0.04
	0.13 - 0.28	6.6A
	0.28 - 0.4	6.9A	20B	9.9	0.17	3.8
	0.65 - 0.75	8.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13
	0.13 - 0.28
	0.28 - 0.4
	0.65 - 0.75
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.28
	0.28 - 0.4
	0.65 - 0.75

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1124	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension