Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1126	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	21/05/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7795271 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	367464  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Mesotrophic Brown Chromosol Thick Non-	Principal Profile Form:	Dy5.41
	gravelly Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Very sparse. *Species includes - Aristida species, Chrysopogon fallax, 
	Heteropogon contortus	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus polycarpa, Bursaria incana, Eucalyptus erythrophloia
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus polycarpa, Eucalyptus 
	erythrophloia
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, subangular, Quartz
	Profile Morphology
	A11	0 - 0.12 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy loam (Light); Massive grade of structure; 
	Sandy (grains prominent) fabric; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to - 
	A12	0.12 - 0.23 m	Brown (10YR4/3-Moist); ; Clayey sand; Massive grade of structure; Earthy fabric; 10-20%, fine 
	gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field 
	pH 6 (Raupach, 0.2); Clear change to - 
	A2	0.23 - 0.5 m	Brown (10YR5/3-Moist); ; Clayey sand; Massive grade of structure; Earthy fabric; 10-20%, fine 
	gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field 
	pH 6.5 (Raupach, 0.45); Clear change to - 
	B21	0.5 - 0.8 m	Light olive brown (2.5Y5/6-Moist); , 7.5YR56, 10-20% , Prominent; , 10-20% ; Sandy light 
	medium clay; Weak grade of structure; Smooth-ped fabric; 2-10%, fine gravelly, 2-6mm, 
	subrounded, Quartz, coarse fragments; Common (10 - 20 %), Ferromanganiferous, Medium (2 -6 
	mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1126	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	6.6A
	0.12 - 0.23	6.8A
	0.25 - 0.5	6.9A
	0.5 - 0.8	6.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.12 - 0.23
	0.25 - 0.5
	0.5 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.23
	0.25 - 0.5
	0.5 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1126	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension