Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1128	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	21/05/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7793339 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	368180  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Reticulate Petroferric Red Kandosol Thick Moderately gravelly	Principal Profile Form:	Dr2.61
	 Sandy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Aristida species, Chrysopogon fallax
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Petalostigma pubescens, Eucalyptus polycarpa, Hakea species
	Tall Strata - Tree, 12.01-20m, Isolated plants. *Species includes - Eucalyptus papuana
	Surface Coarse Fragments:	20-50%, fine gravelly, 2-6mm, subangular, Quartz
	Profile Morphology
	A11	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); ; Clayey sand (Heavy); Massive grade of structure; Sandy (grains 
	prominent) fabric; 10-20%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; 
	A12	0.1 - 0.17 m	Dark reddish brown (5YR3/2-Moist); ; Clayey sand (Heavy); Massive grade of structure; Earthy 
	fabric; 10-20%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.15); 
	A2	0.17 - 0.42 m	Yellowish red (5YR4/6-Moist); ; Clayey sand; Massive grade of structure; Earthy fabric; 10-20%, 
	medium gravelly, 6-20mm, subangular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , 
	; Field pH 6.5 (Raupach, 0.4); 
	B2	0.42 - 0.95 m	Red (10R4/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 50-90%, 
	medium gravelly, 6-20mm, subangular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , 
	; Field pH 6.5 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1128	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1128	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile