Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1138	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	22/05/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	145.695801	Runoff:	No Data
	Easting/Lat.:	-19.5672222	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Reticulate Petroferric Yellow Kandosol Thick Non-gravelly 	Principal Profile Form:	Dy2.51
	Loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Aristida species, Heteropogon contortus, Chrysopogon fallax
	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eucalyptus melanophloia, Melaleuca nervosa
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus polycarpa, Eucalyptus melanophloia, Eucalyptus 
	papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.13 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy loam; Massive grade of structure; Sandy 
	(grains prominent) fabric; Moderately moist; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.1); Clear change to - 
	A12	0.13 - 0.4 m	Brown (10YR5/3-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains prominent) 
	fabric; Moderately moist; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.4); Clear 
	change to - 
	B21	0.4 - 0.8 m	Olive yellow (2.5Y6/6-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric; 
	Moderately moist; Few (2 - 10 %), Ferromanganiferous, Coarse (6 - 20 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.8); Clear change to - 
	B22	0.8 - 0.9 m	Light yellowish brown (2.5Y6/4-Moist); ; Sandy light clay; Massive grade of structure; Earthy 
	fabric; Dry; Many (20 - 50 %), Ferromanganiferous, Coarse (6 - 20 mm), Nodules; , Calcareous, , ;
	 , Gypseous, , ; Field pH 6 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1138	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	5.5A	1.2B	0.43	0.22	0.12
	0.4 - 0.8	5.6A	3B	2.2	0.29	0.29
	0.4 - 0.8	5.6A	3B	2.2	0.29	0.29
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	0.9A	0.02A	58A	26	4	12
	0.4 - 0.8	12	38A	12	3	47
	0.4 - 0.8	12	38A	12	3	47
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.4 - 0.8
	0.4 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1138	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	4A1	pH of 1:5 soil/water suspension
	6A1	Organic carbon - Walkley and Black
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)