Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1141	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	01/06/92	Elevation:	400 metres
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7842382 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	360638  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Rolling low hills 30-90m 10-	Pattern Type:	Hills
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Level
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Kandosol Thick Non-gravelly Loamy 	Principal Profile Form:	Gn2.15
	Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - Cenchrus ciliaris, Aristida species, Heteropogon 
	contortus	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Terminalia oblongata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.15 m	Dark reddish brown (2.5YR3/4-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.03); Clear change to - 
	A12	0.15 - 0.35 m	Dark red (2.5YR3/6-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; , Calcareous,
	 , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.25); Clear change to - 
	B21	0.35 - 1.2 m	Red (10R4/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; , Calcareous, , 
	; , Gypseous, , ; Field pH 5.2 (Raupach, 0.7); Gradual change to - 
	B22	1.2 - 1.6 m	Red (10R4/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; , Calcareous, , 
	; , Gypseous, , ; Field pH 7 (Raupach, 1.4); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1141	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.3A	3.5B	1.4	0.53	0.03
	0.15 - 0.35	6.7A
	0.35 - 1.2	6.8A	2.6B	1.5	0.16	0.03
	1.2 - 1.6	6.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15
	0.15 - 0.35
	0.35 - 1.2
	1.2 - 1.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.35
	0.35 - 1.2
	1.2 - 1.6

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1141	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension