Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1149	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	02/06/92	Elevation:	380 metres
	Map Ref.:	Sheet No. : 8053   GPS	Rainfall:	No Data
	Northing/Long.:	7800586 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	348545  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol Medium Non-gravelly Clay-	Principal Profile Form:	Gn3.1
	loamy Very fine Deep
	ASC Confidence:	Great Soil Group:	Euchrozem
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Dichanthium sericeum, Heteropogon contortus, 
	Chrysopogon fallax	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Surface Coarse Fragments:	0-2%, stony, 200-600mm, rounded, Basalt
	Profile Morphology
	A11	0 - 0.04 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam; Moderate grade of structure, 2-5 mm, Platy; 
	Smooth-ped fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.04); Clear change to 
	- 
	A12	0.04 - 0.15 m	Dark reddish brown (2.5YR3/3-Moist); ; Light clay; Moderate grade of structure, 2-5 mm, Angular 
	blocky; Smooth-ped fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.15); Clear 
	change to - 
	B21	0.15 - 0.4 m	Dark reddish brown (2.5YR3/4-Moist); ; Light medium clay; Moderate grade of structure, 2-5 mm, 
	Angular blocky; Smooth-ped fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	Clear change to - 
	B22	0.4 - 1.3 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Weak grade of structure; Smooth-ped fabric; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1149	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	6.8A
	0.04 - 0.15	6.8A
	0.15 - 0.4	6.9A
	0.4 - 1.3	7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04
	0.04 - 0.15
	0.15 - 0.4
	0.4 - 1.3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.15
	0.15 - 0.4
	0.4 - 1.3

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1149	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension