Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1151	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	02/06/92	Elevation:	380 metres
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7799951 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	346750  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Dermosol Thick Non-gravelly Clayey 	Principal Profile Form:	Uf6.22
	Clayey Deep
	ASC Confidence:	Great Soil Group:	Brown clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Chrysopogon fallax, 
	Dichanthium sericeum	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus tessellaris, Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.06 m	Dark brown (7.5YR3/2-Moist); ; Light clay; Weak grade of structure, 2-5 mm, Polyhedral; Smooth-
	ped fabric; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear change to - 
	A12	0.06 - 0.4 m	Dark brown (7.5YR3/3-Moist); ; Light clay; Weak grade of structure, 2-5 mm, Polyhedral; Smooth-
	ped fabric; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.3); Clear change to - 
	B21	0.4 - 0.5 m	Dark reddish brown (5YR3/2-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm,
	 Angular blocky; Smooth-ped fabric; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules;
	 , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.45); Clear change to - 
	B22	0.5 - 1 m	Brown (7.5YR4/4-Moist); ; Light medium clay; Strong grade of structure, 20-50 mm, Angular 
	blocky; , Lenticular; Smooth-ped fabric; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.9); Clear change to - 
	C	1 - 1.2 m	Brown (7.5YR4/4-Moist); ; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1151	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	7.3A
	0.06 - 0.4	7A
	0.4 - 0.5	7.1A
	0.5 - 1	7.4A
	1 - 1.2	7.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06
	0.06 - 0.4
	0.4 - 0.5
	0.5 - 1
	1 - 1.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.4
	0.4 - 0.5
	0.5 - 1
	1 - 1.2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1151	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension