Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1157	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	03/06/92	Elevation:	360 metres
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7828912 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	352499  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Hypocalcic Brown Dermosol Medium Slightly gravelly 	Principal Profile Form:	Dy2.13
	Clay-loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Dichanthium sericeum, Bothriochloa species, 
	Heteropogon contortus	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus brownii
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, angular, Quartz
	Profile Morphology
	A1	0 - 0.1 m	Very dark grey (10YR3/1-Moist); ; Clay loam, fine sandy; Moderate grade of structure, 20-50 mm, 
	Angular blocky; 10-20%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to - 
	B21	0.1 - 0.5 m	Dark grey (5YR4/1-Moist); ; Medium clay; Weak grade of structure, Angular blocky; Sandy (grains 
	prominent) fabric; 10-20%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.4); Gradual change to - 
	B22	0.5 - 1.15 m	Dark grey (5YR4/1-Moist); ; Medium heavy clay; Weak grade of structure, Angular blocky; Sandy 
	(grains prominent) fabric; 10-20%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; 
	Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Nodules; , Gypseous, , ; Field pH 8.5 (Raupach, 
	1); Clear change to - 
	C	1.15 - 1.25 m	Dark grey (10YR4/1-Moist); ; Medium clay; Massive grade of structure; Earthy fabric; 20-50%, fine
	 gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field 
	pH 8 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1157	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.6A
	0.1 - 0.5	8.4A
	0.5 - 1.15	8.1A
	1.15 - 1.25	7.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.5
	0.5 - 1.15
	1.15 - 1.25
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.5
	0.5 - 1.15
	1.15 - 1.25

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1157	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension