Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1169	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	04/06/92	Elevation:	300 metres
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7798846 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	391862  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached Eutrophic Grey Chromosol Thick Slightly gravelly 	Principal Profile Form:	Dy2.41
	Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax, Dichanthium sericeum, 
	Bothriochloa species	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus crebra
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, rounded, Quartz
	Profile Morphology
	A1	0 - 0.08 m	Dark grey (10YR4/1-Moist); ; Sandy clay loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; 10-20%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to - 
	A2e	0.08 - 0.38 m	Light brownish grey (10YR6/2-Moist); ; Clayey fine sand; Massive grade of structure; Sandy 
	(grains prominent) fabric; 20-50%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.25); 
	B2	0.38 - 0.5 m	Light brownish grey (10YR6/2-Moist); ; Medium clay; Weak grade of structure, 2-5 mm, 
	Polyhedral; Smooth-ped fabric; 20-50%, fine gravelly, 2-6mm, subangular, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.45); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1169	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.4A
	0.08 - 0.38	6.5A
	0.35 - 0.5	6.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.38
	0.35 - 0.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.38
	0.35 - 0.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1169	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension