Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1179	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	05/06/92	Elevation:	320 metres
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7792038 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	379671  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Black Dermosol Moderately gravelly Clayey 	Principal Profile Form:	Uf6.32
	Clayey Deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Eulalia aurea, Bothriochloa species, Dichanthium 
	species	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	20-50%, fine gravelly, 2-6mm, subrounded, Quartz
	Profile Morphology
	A11	0 - 0.05 m	Very dark grey (10YR3/1-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Polyhedral; 
	Smooth-ped fabric; 10-20%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to - 
	B21	0.05 - 0.25 m	Dark grey (10YR4/1-Moist); ; Medium clay (Heavy); Moderate grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; 20-50%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.15); Gradual change to - 
	B22	0.25 - 1 m	Very dark grey (10YR3/1-Moist); ; Medium heavy clay; Weak grade of structure; Smooth-ped 
	fabric; 20-50%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.5); Gradual change to - 
	B23	1 - 1.4 m	Yellowish brown (10YR5/4-Moist); Mottles, 10YR41, 10-20% , Faint; Mottles, 10-20% ; Medium 
	heavy clay; Weak grade of structure; Smooth-ped fabric; 10-20%, fine gravelly, 2-6mm, 
	subrounded, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 4.5 (Raupach, 
	1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1179	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.4A	3B	3.7	0.19	0.23
	0.05 - 0.25	6.1A
	0.25 - 1	4.9A	5.4B	7.2	0.06	8
	1 - 1.4	4.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.25
	0.25 - 1
	1 - 1.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.25
	0.25 - 1
	1 - 1.4

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1179	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension